For 1990-2009 cars

Table 1: | X102
Table 2: | X102
Table 3: | X104
Table 4: | X104
Table 5: | X106
Table 6: | X106
Table 7: | X108
Table 8: | X108
Table 9: | X110
Table 10: | X110
Table 11: | X112
Table 12: | X112
Table 13: | X113
Table 14: | X113
Table 15: | X114
Table 16: | X114
Table 17: | X160
Table 18: | X160
Table 19: | X161
Table 20: | X161
Table 21: | X162
Table 22: | X162
Table 23: | X200
Table 24: | X200
Table 25: | X201
Table 26: | X201
Table 27: | X202
Table 28: | X202
Table 29: | X203
Table 30: | X203
Table 31: | X204
Table 32: | X204
Table 33: | X205
Table 34: | X205
Table 35: | X206
Table 36: | X206
Table 37: | X207
Table 38: | X207
Table 39: | X210
Table 40: | X210
Table 41: | X212
Table 42: | X212
Table 43: | X223
Table 44: | X223
Table 45: | X227
Table 46: | X227
Table 47: | X241
Table 48: | X241
Table 49: | X253
Table 50: | X253
Table 51: | X254
Table 52: | X254
Table 53: | X303
Table 54: | X303
Table 55: | X304
Table 56: | X304
Table 57: | X305
Table 58: | X305
Table 59: | X309
Table 60: | X309
Table 61: | X311
Table 62: | X311
Table 63: | X315
Table 64: | X315
Table 65: | X328
Table 66: | X328
Table 67: | X355
Table 68: | X355
Table 69: | X356
Table 70: | X356
Table 71: | X360
Table 72: | X360

#### X102

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 450 | 3.6L: Ground
BK | 450 | 6.0L: Ground
2 | D-GN | 335 | 6.0L-Low Speed Cooling Fan Relay Control
OG/YE | 3640 | 4L60/5L40: Battery Positive Voltage
3 | D-BU | 1225 | 4L60: Transmission Fluid Pressure Switch Signal B
BN | 5069 | 6.0L: Main Relay Control
4 | -- | -- | Not Used
5 | PK/D-BU | 5290 | 6.0L: Ignition 1 Voltage
OG/BK | 540 | 3.6L: Battery Positive Voltage
6 | BK | 350 | 3.6L: Ground
7 | OG | 1525 | 5L40: Clutch Pressure Control Solenoid Valve 1 High Control
OG | 1226 | 4L60: Transmission Fluid Pressure Switch Signal C
8 | L-BU/WH | 1229 | 4L60: PC Solenoid Valve Low Control
BK | 350 | 6.0L: Ground
9 | D-BU | 7393 | AC Compressor Low Reference
10 | PK | 439 | 3.6L : Ignition 1 Voltage
D-BU/BK | 473 | High Speed Cooling Fan Relay Control
11 | BN/WH | 2762 | 5L40: Low Reference
12 | BN | 2501 | 3.6L/6L50: High Speed GMLAN Serial Data Bus-
13 | D-GN | 7392 | AC Compressor Supply Voltage
14 | L-BU | 1937 | 3.6L: Fuel Level Sensor Signal (Secondary)
RD/BK | 1786 | 6.0L: Park/Neutral Signal
15 | D-GN/WH | 465 | 3.6L: Fuel Pump Relay Control
D-BU | 5985 | 6L50: TCM Accessory Signal
16 | OG/WH | 3223 | 6.0L: HO2S Heater Low Control (Bank 2 Sensor 2)
BN/YE | 452 | 3.6L: Low Reference)
17 | BN/BK | 2500 | 3.6L/6L50: High Speed GMLAN Serial Data Bus+
18 | PU | 1589 | 3.6L: Fuel Level Sensor Signal (Primary)
BN | 2501 | 6L50: High Speed GMLAN Serial Data Bus-
19 | BN | 1271 | 3.6L: Low Reference
WH/BU | 17 | 6L50: Stop Lamp Switch Signal
20 | BU/WH | 1161 | 3.6L: APP Sensor 1 Signal
BN | 3122 | 6.0L: HO2S Heater Low Control (Bank 1 Sensor 2)
21 | WH/BK | 1164 | 3.6L: 5-Volt Reference
PU | 1670 | 6.0L: HO2S High Signal (Bank 2 Sensor 2)
22 | L-BU | 1162 | 3.6L: APP Sensor 2 Signal
BN/WH | 1671 | 6.0L: HO2S Low Signal (Bank 2 Sensor 2)
23 | BN/YE | 1274 | 3.6L: 5-Volt Reference
BN/BK | 2500 | 6L50: High Speed GMLAN Serial Data Bus+
24 | PU | 1272 | 3.6L: Low Reference
PU/WH | 1668 | 6.0L: HO2S High Signal (Bank 1 Sensor 2)
25 | BN/WH | 419 | 3.6L: MIL Control
BN/WH | 1669 | 6.0L: HO2S Low Signal (Bank 1 Sensor 2)
26 | OG/YE | 6109 | Clutch Pedal Position Sensor Reference
OG/BK | 1228 | 5L40: PC Solenoid Valve High Control
BN/RD | 472 | 6.0L: IAT Sensor Signal
27 | YE | 6111 | 3.6L Manual: Clutch Pedal Position Sensor Signal
L-BU/WH | 1229 | 5L40: PC Solenoid Valve Low Control
YE | 492 | 6.0L: MAF Sensor Signal
28 | PU/WH | 821 | 4L60: OSS High Signal
L-GN/BK | 822 | 5L40: VSS High Signal
OG/BK | 380 | 6.0L: A/C Refrigerant Pressure Sensor Signal
29 | PK | 1224 | 4L60: Transmission Fluid Pressure Switch Signal A
GY | 2709 | 6.0L: 5-Volt Reference
30 | BN/OG | 422 | 4L60: TCC Solenoid Valve Control
WH/BU | 17 | 5L40: Stop Lamp Switch Signal
PK | 439 | 6.0L: Ignition 1 Voltage
31 | YE/BK | 1227 | 4L60/5L40: TFT Sensor Signal
BN/WH | 2760 | 6.0L: Low Reference
32 | L-GN | 5007 | 6.0L: Backup Lamp Switch Signal
L-BU | 1984 | 4L60/5L40: Transmission Turbine Speed Switch Low Reference
-- | -- | Not Used
33 | L-GN/BK | 822 | 4L60: OSS Low Signal
PK/WH | 821 | 5L40: VSS Low Signal
BN/D-GN | 2759 | 6.0L: Low Reference
34 | WH/GN | 687 | 4L60: 3-2 Shift Solenoid Valve Control
WH | 898 | Shift Solenoid C Valve Control
35 | BK/YE | 1223 | 4L60/5L40 Shift Solenoid B Valve Control
36 | L-GN | 1222 | 4L60/5L40 Shift Solenoid A Valve Control
37 | OG | 1983 | 4L60/5L40 Transmission Turbine Speed Switch Signal
38 | WH | 776 | 4L60/5L40 Transmission Range Switch Signal P
39 | GY | 773 | 4L60/5L40 Transmission Range Switch Signal C
40 | YE | 772 | 4L60/5L40 Transmission Range Switch Signal B
41 | BN/YE | 771 | 4L60/5L40 Transmission Range Switch Signal A
42 | BN | 418 | 4L60/5L40 TCC PWM Solenoid Valve Control

#### X102

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 450 | 3.6L: Ground
BK | 450 | 6.0L: Ground
2 | D-GN | 335 | 6.0L-Low Speed Cooling Fan Relay Control
OG/YE | 3640 | 4L60/5L40: Battery Positive Voltage
3 | D-BU | 1225 | 4L60: Transmission Fluid Pressure Switch Signal B
BN | 5069 | 6.0L: Main Relay Control
4 | -- | -- | Not Used
5 | PK/BU | 2590 | 6.0L: Ignition 1 Voltage
OG/BK | 540 | 3.6L: Battery Positive Voltage
6 | BK | 250 | 3.6L: Ground
7 | OG | 1525 | 5L40: Clutch Pressure Control Solenoid Valve 1 High Control
OG | 1226 | 4L65/4L60: Transmission Fluid Pressure Switch Signal C
8 | L-BU/WH | 1229 | 4L60: PC Solenoid Valve Low Control
BK | 350 | 6.0L: Ground
9 | D-BU | 7393 | AC Compressor Low Reference
10 | PK | 439 | 3.6L : Ignition 1 Voltage
D-BU/BK | 473 | High Speed Cooling Fan Relay Control
11 | BN/WH | 2762 | 5L40: Low Reference
12 | BN | 2501 | 3.6L/6L50: High Speed GMLAN Serial Data Bus-
13 | D-GN | 7392 | AC Compressor Supply Voltage
14 | L-BU | 1937 | 3.6L: Fuel Level Sensor Signal (Secondary)
RD/BK | 1786 | 6.0L: Park/Neutral Signal
15 | D-GN/WH | 465 | 3.6L: Fuel Pump Relay Control
D-BU | 1585 | 6L50: TCM Accessory Signal
16 | OG/WH | 3223 | 6.0L: HO2S Heater Low Control (Bank 2 Sensor 2)
BN/YE | 452 | 3.6L: Low Reference)
17 | BN/BK | 2500 | 3.6L/6L50: High Speed GMLAN Serial Data Bus+
18 | PU | 1589 | 3.6L: Fuel Level Sensor Signal (Primary)
BN | 2501 | 6L50: High Speed GMLAN Serial Data Bus-
19 | BN | 1271 | 3.6L: Low Reference
WH/BU | 17 | 6L50: Stop Lamp Switch Signal
20 | BU/WH | 1161 | 3.6L: APP Sensor 1 Signal
BN | 3122 | 6.0L: HO2S Heater Low Control (Bank 1 Sensor 2)
21 | WH/BK | 1164 | 3.6L: 5-Volt Reference
PU | 1670 | 6.0L: HO2S High Signal (Bank 2 Sensor 2)
22 | L-BU | 1162 | 3.6L: APP Sensor 2 Signal
BN/WH | 1671 | 6.0L: HO2S Low Signal (Bank 2 Sensor 2)
23 | BN/YE | 1274 | 3.6L: 5-Volt Reference
BN/BK | 2500 | 6L50: High Speed GMLAN Serial Data Bus+
24 | PU | 1272 | 3.6L: Low Reference
PU/WH | 1668 | 6.0L: HO2S High Signal (Bank 1 Sensor 2)
25 | BN/WH | 419 | 3.6L: MIL Control
BN/WH | 1669 | 6.0L: HO2S Low Signal (Bank 1 Sensor 2)
26 | OG/YE | 6109 | Clutch Pedal Position Sensor Reference
OG/BK | 1228 | 5L40: PC Solenoid Valve High Control
BN/RD | 472 | 6.0L: IAT Sensor Signal
27 | YE | 6111 | 3.6L Manual: Clutch Pedal Position Sensor Signal
L-BU/WH | 1229 | 5L40: PC Solenoid Valve Low Control
YE | 492 | 6.0L MAF Sensor Signal
28 | PU/WH | 821 | 4L60: OSS High Signal
L-GN/BK | 822 | 5L40: VSS High Signal
OG/BK | 380 | 6.0L: A/C Refrigerant Pressure Sensor Signal
29 | PK | 1224 | 4L60: Transmission Fluid Pressure Switch Signal A
GY | 2709 | 6.0L: 5-Volt Reference
30 | BN/OG | 422 | 4L60: TCC Solenoid Valve Control
WH/BU | 17 | 5L40: Stop Lamp Switch Signal
PK | 439 | 6.0L: Ignition 1 Voltage
31 | YE/BK | 1227 | 4L60/5L40: TFT Sensor Signal
BN/WH | 2760 | 6.0L: Low Reference
32 | L-GN | 2007 | 6.0L: Backup Lamp Switch Signal
L-BU | 1984 | 4L60/5L40: Transmission Turbine Speed Switch Low Reference
33 | L-GN/BK | 822 | 4L60: OSS Low Signal
PK/WH | 821 | 5L40: VSS Low Signal
BN/D-GN | 2759 | 6.0L: Low Reference
34 | WH/GN | 687 | 4L60: 3-2 Shift Solenoid Valve Control
WH | 898 | 5L40: Shift Solenoid C Valve Control
35 | YE/BK | 1223 | 4L60/5L40 Shift Solenoid B Valve Control
36 | L-GN | 1222 | 4L60/5L40 Shift Solenoid A Valve Control
37 | OG | 1983 | 4L60/5L40 Transmission Turbine Speed Switch Signal
38 | WH | 776 | 4L60/5L40 Transmission Range Switch Signal P
39 | GY | 773 | 4L60/5L40 Transmission Range Switch Signal C
40 | YE | 772 | 4L60/5L40 Transmission Range Switch Signal B
41 | BN/YE | 771 | 4L60/5L40 Transmission Range Switch Signal A
42 | BN | 418 | 4L60/5L40 TCC PWM Solenoid Valve Control

#### X104

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | BN/YE | 6110 | Clutch Pedal Position Sensor Return
3 | D-BU | 7393 | AC Compressor Low Reference
4 | D-GN | 7392 | AC Compressor Supply Voltage
5 | PK/BU | 1339 | Ignition 1 Voltage
6 | -- | -- | Not Used
7 | OG/YE | 6901 | Clutch pedal position Reference
8 | YE | 6111 | Clutch pedal position Signal
9 | BN/YE | 1969 | Headlamp High Beam Relay Control
10 | L-BU | 1162 | APP Sensor 2 Signal
11 | OG/GN | 2240 | Battery Positive Voltage
12 | WH/YE | 1080 | Park Lamp Relay Control
13 | PK/WH | 1970 | Headlamp Low Beam Relay Control
14 | D-GN/WH | 465 | Fuel Pump Relay Control
15 | D-GN | 646 | Backup Lamp Relay Control
16 | PU | 5531 | Hood Closed Switch Signal
17 | BN/BK | 28 | Horn Relay Control
18 | PK/BK | 109 | Hood Ajar Switch Signal
19 | PU/WH | 5727 | Communication Enable Relay Control
20 | GY | 91 | Windshield Wiper Switch Signal 2
21 | BN/WH | 33 | Brake Warning Indicator Control
22 | YE | 196 | Windshield Wiper Motor Park Switch Signal
23 | BN/RD | 860 | Front Windshield Wiper Switch High Signal
24 | D-BU | 5985 | TCM Accessory Signal
25 | PK | 1439 | Run/Crank Control
26 | WH/BU | 193 | Rear Defog Relay Control
27 | BN | 2501 | High Speed GMLAN Serial Data Bus-
28 | BN/WH | 419 | MIL Control
29 | OG | 2268 | Washer Fluid Pump Relay Control
30 | L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage
31 | -- | -- | Not Used
32 | BN/BK | 2500 | High Speed GMLAN Serial Data Bus+
33 | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage
34 | WH/BU | 17 | Stop Lamp Switch Signal
35 | BN/YE | 1274 | 5-Volt Reference
36 | -- | -- | Not Used
37 | -- | -- | Not Used
38 | PU | 1272 | Low Reference
39 | BU/WH | 1161 | APP Sensor 1 Signal
40 | WH/BK | 1164 | 5-Volt Reference
41 | BN | 1271 | Low Reference
42 | - | - | Not Used

#### X104

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | BN/YE | 6110 | Clutch Pedal Position Sensor Return
3 | D-BU | 7393 | AC Compressor Low Reference
4 | D-GN | 7392 | AC Compressor Supply Voltage
5 | PK/BU | 1339 | Ignition 1 Voltage
6 | -- | -- | Not Used
7 | OG/YE | 6901 | Clutch pedal position Reference
8 | YE | 6111 | Clutch pedal position Signal
9 | BN/YE | 1969 | Headlamp High Beam Relay Control
10 | L-BU | 1162 | APP Sensor 2 Signal
11 | OG/GN | 2240 | Battery Positive Voltage
12 | WH/YE | 1080 | Park Lamp Relay Control
13 | PK/WH | 1970 | Headlamp Low Beam Relay Control
14 | D-GN/WH | 465 | Fuel Pump Relay Control
15 | D-GN | 646 | Backup Lamp Relay Control
16 | PU | 5331 | Hood Closed Switch Signal
17 | BN/BK | 28 | Horn Relay Control
18 | PK/BK | 109 | Hood Ajar Switch Signal
19 | PU/WH | 5727 | Communication Enable Relay Control
20 | GY | 91 | Windshield Wiper Switch Signal 2
21 | BN/WH | 33 | Brake Warning Indicator Control
22 | YE | 196 | Windshield Wiper Motor Park Switch Signal
23 | BN/RD | 860 | Front Windshield Wiper Switch High Signal
24 | D-BU | 5985 | TCM Accessory Signal
25 | PK | 1439 | Run/Crank Control
26 | WH/BU | 193 | Rear Defog Relay Control
27 | BN | 2501 | High Speed GMLAN Serial Data Bus-
28 | BN/WH | 419 | MIL Control
29 | OG | 2268 | Washer Fluid Pump Relay Control
30 | L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage
31 | -- | -- | Not Used
32 | BN/BK | 2500 | High Speed GMLAN Serial Data Bus+
33 | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage
34 | WH/BU | 17 | Stop Lamp Switch Signal
35 | BN/YE | 1274 | 5-Volt Reference
36 | -- | -- | Not Used
37 | -- | -- | Not Used
38 | PU | 1272 | Low Reference
39 | BU/WH | 1161 | APP Sensor 1 Signal
40 | WH/BK | 1164 | 5-Volt Reference
41 | BN | 1271 | Low Reference
42 | BN | 418 | 4L60/5L40 TCC PWM Solenoid Valve Control

#### X106

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | -- | -- | Not Used
B | BK | 350 | Ground
C | -- | -- | Not Used
D | D-GN | 1409 | Discriminating Sensor - Signal
E | GY | 5600 | Discriminating Sensor - Low Reference
F | -- | -- | Not Used
G | -- | -- | Not Used
H | YE | 354 | Discriminating Sensor - Signal
J | BN/YE | 5045 | Discriminating Sensor - Low Reference
K | -- | -- | Not Used
L | -- | -- | Not Used
M | - | - | Not Used

#### X106

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | -- | -- | Not Used
B | BK | 350 | Ground
C | -- | -- | Not Used
D | D-GN | 1409 | Discriminating Sensor - Signal
E | GY | 5600 | Discriminating Sensor - Low Reference
F | -- | -- | Not Used
G | -- | -- | Not Used
H | YE | 354 | Discriminating Sensor - Signal
J | BN/YE | 5045 | Discriminating Sensor - Low Reference
K | -- | -- | Not Used
L | -- | -- | Not Used
M | -- | -- | Not Used

#### X108

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | -- | -- | Not Used
3 | -- | -- | Not Used
4 | PU | 34 | Fog Lamps Supply Voltage
5 | -- | -- | Not Used
6 | -- | -- | Not Used
7 | -- | -- | Not Used
8 | BK | 350 | Ground

#### X108

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | -- | -- | Not Used
3 | -- | -- | Not Used
4 | PU | 34 | Fog Lamps Supply Voltage
5 | -- | -- | Not Used
6 | -- | -- | Not Used
7 | -- | -- | Not Used
8 | BK | 350 | Ground

#### X110

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | RD/BK | 142 | Battery Positive Voltage
2 | OG | 3540 | Battery Positive Voltage

#### X110

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | RD/BK | 142 | Battery Positive Voltage
2 | OG | 3540 | Battery Positive Voltage

#### X112

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2650 | Ground
B | OG/WH | 2122 | Ignition Control 2
C | D-GN | 2124 | Ignition Control 4
E | BN/WH | 2130 | Low Reference
F | L-BLU/WH | 2126 | Ignition Control 6
G | PU/WH | 2128 | Ignition Control 8
H | PK/BK | 5292 | Ignition 1 Voltage

#### X112

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2650 | Ground
B | OG/WH | 2122 | Ignition Control 2
C | D-GN/WH | 2124 | Ignition Control 4
E | BN/WH | 2130 | Low Reference
F | L-BU/WH | 2126 | Ignition Control 6
G | PU/WH | 2128 | Ignition Control 8
H | PK | 5292 | Ignition 1 Voltage

#### X113

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2450 | Ground
B | OG | 2127 | Ignition Control 7
C | D-GN | 2125 | Ignition Control 5
E | BN | 2129 | Low Reference
F | L-BU | 2123 | Ignition Control 3
G | PU | 2121 | Ignition Control 1
H | PK/BK | 5291 | Ignition 1 Voltage

#### X113

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
A | BK | 2450 | Ground
B | OG | 2127 | Ignition Control 7
C | D-GN/RD | 2125 | Ignition Control 5
E | BN | 2129 | Low Reference
F | L-BU | 2123 | Ignition Control 3
G | PU | 2121 | Ignition Control 1
H | PK/BU | 5291 | Ignition 1 Voltage

#### X114

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/BU | 5291 | Ignition 1 Voltage
2 | PK | 5292 | Ignition 1 Voltage
3 | BN/BK | 1744 | Fuel Injector 1 Control
4 | PK/BK | 1746 | Fuel Injector 3 Control
5 | BN/WH | 845 | Fuel Injector 5 Control
6 | L-GN/BK | 1745 | Fuel Injector 2 Control
7 | L-BU/BK | 844 | Fuel Injector 4 Control
8 | YE/BK | 846 | Fuel Injector 6 Control
9 | -- | -- | Not Used
10 | -- | -- | Not Used

#### X114

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/BU | 5291 | Ignition 1 Voltage
2 | PK | 5292 | Ignition 1 Voltage
3 | BN/BK | 1744 | Fuel Injector 1 Control
4 | PK/BK | 1746 | Fuel Injector 3 Control
5 | BN/WH | 845 | Fuel Injector 5 Control
6 | L-GN/BK | 1745 | Fuel Injector 2 Control
7 | L-BU/BK | 844 | Fuel Injector 4 Control
8 | YE/BK | 846 | Fuel Injector 6 Control
9 | -- | -- | Not Used
10 | -- | -- | Not Used

#### X160

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | L-BU | 830 | Left Front Wheel Speed Sensor Signal
2 | GY | 7064 | Left Front Wheel Speed Sensor Supply Voltage

#### X160

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN | 830 | Left Front Wheel Speed Sensor Signal
2 | BK | 7064 | Left Front Wheel Speed Sensor Supply Voltage

#### X161

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | D-GN | 872 | Right Front Wheel Speed Sensor Signal
2 | GY | 7065 | Right Front Wheel Speed Sensor Supply Voltage

#### X161

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN | 872 | Right Front Wheel Speed Sensor Signal
2 | BK | 7065 | Right Front Wheel Speed Sensor Supply Voltage

#### X162

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BU | 409 | Left Cooling Fan Motor Supply Voltage
2 | BK | 250 | Ground
3 | WH | 504 | Right Cooling Fan Motor Supply Voltage
4 | GY | 532 | Right Cooling Fan Motor Low Reference

#### X162

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BU | 409 | Left Cooling Fan Motor Supply Voltage
2 | BK | 250 | Ground
3 | WH | 504 | Right Cooling Fan Motor Supply Voltage
4 | GY | 532 | Right Cooling Fan Motor Low Reference

#### X200

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | RD | 242 | Battery Positive Voltage
2 | RD/BK | 642 | Battery Positive Voltage

#### X200

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | RD | 242 | Battery Positive Voltage
2 | RD/BK | 642 | Battery Positive Voltage

#### X201

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | -- | -- | Not Used
3 | -- | -- | Not Used
4 | -- | -- | Not Used
5 | -- | -- | Not Used
6 | GY/BK | 745 | Right Front Door Ajar Switch Signal
7 | -- | -- | Not Used
8 | -- | -- | Not Used
9 | -- | -- | Not Used
10 | -- | -- | Not Used
11 | -- | -- | Not Used
12 | -- | -- | Not Used
13 | -- | -- | Not Used
14 | -- | -- | Not Used
15 | -- | -- | Not Used
16 | L-BU | 20 | Not Used
17 | OG/BK | 233 | Park Brake Switch Signal
18 | -- | -- | Not Used
19 | L-BU | 5986 | Communication Enable Relay Supply Voltage
20 | -- | -- | Not Used
21 | -- | -- | Not Used
22 | -- | -- | Not Used
23 | -- | -- | Not Used
24 | -- | -- | Not Used
25 | -- | -- | Not Used
26 | L-GN/WH | 512 | Right Front Low Level Audio Signal (+)
27 | YE | 6817 | LED Backlight Dimming Control
28 | OG/BU | 1540 | Battery Positive Voltage
29 | BK/BU | 2088 | Yaw Rate Sensor Return
30 | PK | 781 | Driver Door Lock Switch Unlock Signal
31 | D-BU/WH | 149 | Courtesy Lamps Supply Voltage
32 | -- | 0.5 | Not Used
33 | -- | -- | Not Used
34 | -- | -- | Not Used
35 | -- | -- | Not Used
36 | BN/OG | 511 | Left Front Low Level Audio Signal (+)
37 | D-GN/WH | 1317 | Fog Lamp Relay Control
38 | GY | 8 | Instrument Panel Lamp Supply Voltage
39 | -- | -- | Not Used
40 | PK/BK | 780 | Driver Door Lock Switch Lock Signal
41 | YE/BK | 1334 | Left Rear Turn Signal Lamp Supply Voltage
42 | D-GN/WH | 1335 | Right Rear Turn Signal Lamp Supply Voltage
43 | L-GN | 24 | Backup Lamp Supply Voltage

#### X201

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | -- | -- | Not Used
3 | -- | -- | Not Used
4 | -- | -- | Not Used
5 | -- | -- | Not Used
6 | GY/BK | 745 | Right Front Door Ajar Switch Signal
7 | -- | -- | Not Used
8 | -- | -- | Not Used
9 | -- | -- | Not Used
10 | BN/RD | 694 | Driver Door Lock Actuator Unlock Control
11 | -- | -- | Not Used
12 | -- | -- | Not Used
13 | -- | -- | Not Used
14 | -- | -- | Not Used
15 | -- | -- | Not Used
16 | L-BU | 20 | Stop Lamp Switch Signal
17 | OG/BK | 233 | Park Brake Switch Signal
18 | -- | -- | Not Used
19 | L-BU | 5986 | Communication Enable Relay Supply Voltage
20 | -- | -- | Not Used
21 | -- | -- | Not Used
22 | -- | -- | Not Used
23 | -- | -- | Not Used
24 | -- | -- | Not Used
25 | -- | -- | Not Used
26 | L-GN/WH | 512 | Right Front Low Level Audio Signal (+)
27 | YE | 6817 | LED Backlight Dimming Control
28 | OG/BU | 1540 | Battery Positive Voltage
29 | BK/BU | 2088 | Yaw Rate Sensor Return
30 | PK | 781 | Driver Door Lock Switch Unlock Signal
31 | D-BU/WH | 149 | Courtesy Lamps Supply Voltage
32 | -- | -- | Not Used
33 | -- | -- | Not Used
34 | -- | -- | Not Used
35 | -- | -- | Not Used
36 | BN/OG | 511 | Left Front Low Level Audio Signal (+)
37 | D-GN/WH | 1317 | Fog Lamp Relay Control
38 | GY | 8 | Instrument Panel Lamp Supply Voltage
39 | -- | -- | Not Used
40 | PK/BK | 780 | Driver Door Lock Switch Lock Signal
41 | YE/BK | 1334 | Left Rear Turn Signal Lamp Supply Voltage
42 | D-GN/WH | 1335 | Right Rear Turn Signal Lamp Supply Voltage
43 | L-GN | 24 | Backup Lamp Supply Voltage

#### X202

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/GN | 2840 | Battery Positive Voltage
2 | -- | -- | Not Used
3 | -- | -- | Not Used
4 | BN | 201 | Base: Left Front Speaker Output (+)
5 | GY | 118 | Base: Left Front Speaker Output (-)
6 | BN/WH | 243 | Accessory Voltage
7 | GN/WH | 295 | Door Lock Actuator Lock Control
8 | -- | -- | Not Used
9 | BN/BU | 343 | Accessory Voltage
10 | PK | 5076 | 5-Volt Reference
11 | BN | 5077 | Low Reference
12 | BN/BK | 254 | Power Door Unlock Fuse Supply Voltage
13 | BN/WH | 746 | Passenger Door Ajar Switch Control
14 | OG/BU | 2440 | Battery Positive Voltage
15 | OG/WH | 2340 | Battery Positive Voltage
16 | BN/RD | 294 | Door Lock Actuator Unlock Control
17 | BN/YE | 143 | Accessory Voltage
18 | OG/YE | 4540 | Battery Positive Voltage
19 | -- | -- | Not Used
20 | -- | -- | Not Used
21 | WH/GN | 5075 | Battery Current Signal
22 | -- | -- | Not Used
23 | OG/WH | 1840 | Battery Positive Voltage
24 | BK | 1650 | Ground
25 | -- | -- | Not Used
26 | OG/BU | 4340 | Battery Positive Voltage
27 | -- | -- | Not Used
28 | GY | 120 | Fuel Pump Supply Voltage
29 | OG | 1140 | Battery Positive Voltage
30 | -- | -- | Not Used
31 | -- | -- | Not Used
32 | -- | -- | Not Used
33 | -- | -- | Not Used
34 | D-GN | 5060 | Low Speed GMLAN Serial Data
35 | GY/BK | 255 | Power Door Lock Fuse Supply Voltage
36 | D-GN | 1301 | Rap (X) Fuse Supply Voltage
37 | OG/YE | 1340 | Battery Positive Voltage
38 | D-GN | 1001 | Rap (X) Fuse Supply Voltage

#### X202

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/GN | 2840 | Battery Positive Voltage
2 | -- | -- | Not Used
3 | -- | -- | Not Used
4 | BN | 201 | Base: Left Front Speaker Output (+)
5 | GY | 118 | Base: Left Front Speaker Output (-)
6 | BN/WH | 243 | Accessory Voltage
7 | GN/WH | 295 | Door Lock Actuator Lock Control
8 | -- | -- | Not Used
9 | BN/BU | 343 | Accessory Voltage
10 | PK | 5076 | 5-Volt Reference
11 | BN | 5077 | Low Reference
12 | BN/BK | 254 | Power Door Unlock Fuse Supply Voltage
13 | BN/WH | 746 | Passenger Door Ajar Switch Control
14 | OG/BU | 2440 | Battery Positive Voltage
15 | OG/WH | 2340 | Battery Positive Voltage
16 | BN/RD | 294 | Door Lock Actuator Unlock Control
17 | BN/YE | 143 | Accessory Voltage
18 | -- | -- | Not Used
19 | -- | -- | Not Used
20 | -- | -- | Not Used
21 | WH/GN | 5075 | Battery Current Signal
22 | -- | -- | Not Used
23 | OG/WH | 1840 | Battery Positive Voltage
24 | BK | 1650 | Ground
25 | OG/PU | 2140 | Battery Positive Voltage
26 | OG/BU | 4340 | Battery Positive Voltage
27 | -- | -- | Not Used
28 | GY | 120 | Fuel Pump Supply Voltage
29 | OG | 1140 | Battery Positive Voltage
30 | -- | -- | Not Used
31 | -- | -- | Not Used
32 | -- | -- | Not Used
33 | -- | -- | Not Used
34 | D-GN | 5060 | Low Speed GMLAN Serial Data
35 | GY/BK | 255 | Power Door Lock Fuse Supply Voltage
36 | D-GN | 1301 | Rap (X) Fuse Supply Voltage
37 | OG/YE | 1340 | Battery Positive Voltage
38 | D-GN | 1001 | Rap (X) Fuse Supply Voltage

#### X203

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | L_BU | 5986 | Communication Enable Relay Supply Voltage
2 | BK/BU | 2088 | Steering Wheel Position Sensor Low Reference
3 | -- | -- | Not Used
4 | BN | 185 | Low Washer Fluid Indicator Control
5 | -- | -- | Not Used
6 | WH | 2282 | Headlamp Washer Relay Control
7 | BN | 61 | Low Reference
8 | L_GN/BK | 735 | Ambient Air Temperature Sensor Signal

#### X203

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | L_BU | 5986 | Communication Enable Relay Supply Voltage
2 | BK/BU | 2088 | Steering Wheel Position Sensor Low Reference
3 | -- | -- | Not Used
4 | BN | 185 | Low Washer Fluid Indicator Control
5 | -- | -- | Not Used
6 | WH | 2282 | Headlamp Washer Relay Control
7 | BN | 61 | Low Reference
8 | L_GN/BK | 735 | Ambient Air Temperature Sensor Signal

#### X204

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | GN | 442 | Battery Positive Voltage

#### X204

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | GN | 442 | Battery Positive Voltage

#### X205

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG | 1732 | Courtesy Lamps Supply Voltage
2 | -- | -- | Not Used
3 | BK/WH | 1450 | Ground
4 | -- | -- | Not Used
5 | -- | -- | Not Used
6 | D-BU | 6189 | Rear Compartment Relay Switch
7 | -- | -- | Not Used
8 | -- | -- | Not Used
9 | -- | -- | Not Used
10 | OG/WH | 2340 | Battery Positive Voltage
11 | BK/WH | 1051 | Ground
12 | L-GN | 5060 | Low Speed GMLAN Serial Data
13 | PK/BK | 2062 | Navigation Mono Audio Signal (+)
14 | OG/BK | 2061 | Navigation Mono Audio Signal (-)
15 | -- | -- | Not Used

#### X205

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG | 1732 | Courtesy Lamps Supply Voltage
2 | -- | -- | Not Used
3 | BK/WH | 1450 | Ground
4 | -- | -- | Not Used
5 | -- | -- | Not Used
6 | -- | -- | Not Used
7 | -- | -- | Not Used
8 | -- | -- | Not Used
9 | -- | -- | Not Used
10 | OG/WH | 2340 | Battery Positive Voltage
11 | BK/WH | 1051 | Ground
12 | L-GN | 5060 | Low Speed GMLAN Serial Data
13 | PK/BK | 2062 | Navigation Mono Audio Signal (+)
14 | OG/BK | 2061 | Navigation Mono Audio Signal (-)
15 | -- | -- | Not Used

#### X206

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PU | 293 | Rear Defog Element Supply Voltage
2 | -- | -- | Not Used
3 | L-GN | 24 | Backup Lamp Supply Voltage
4 | -- | -- | Not Used
5 | -- | -- | Not Used
6 | L-BU | 1937 | Fuel Level Signal (Secondary)
7 | BN/WH | 309 | Lamp Supply Voltage
8 | -- | -- | Not Used
9 | -- | -- | Not Used
10 | -- | -- | Not Used
11 | -- | -- | Not Used
12 | PU | 709 | Left Park Lamp Supply Voltage
13 | PK/BU | 339 | Ignition 1 Voltage
14 | -- | -- | Not Used
15 | -- | -- | Not Used
16 | -- | -- | Not Used
17 | BN/BK | 884 | Left Rear Wheel Speed Sensor Signal
18 | GY | 7128 | Right Rear Wheel Speed Sensor Supply Voltage
19 | BN/YE | 452 | Low Reference
20 | GY | 5600 | Discriminating Sensor - Low Reference
21 | YE | 354 | Discriminating Sensor - Signal
22 | D-GN/WH | 1317 | Fog Lamp Relay Control
23 | BN/WH | 2086 | Yaw Rate Sensor Test Control
24 | -- | -- | Not Used
25 | -- | -- | Not Used
26 | -- | -- | Not Used
27 | -- | -- | Not Used
28 | OG/BK | 540 | Battery Positive Voltage
29 | -- | -- | Not Used
30 | -- | -- | Not Used
31 | GY | 7127 | Left Rear Wheel Speed Sensor Supply Voltage
32 | BN | 882 | Right Rear Wheel Speed Sensor Signal
33 | PU | 1589 | Fuel Level Sensor Signal (Primary)
34 | D-GN | 1409 | Discriminating Sensor - Signal
35 | BN/YE | 5045 | Discriminating Sensor - Low Reference
36 | D-GN | 2087 | Steering Wheel Position Sensor 5-V Reference
37 | L-GN/BK | 5352 | Yaw Rate Sensor Test Control
38 | PU/WH | 1699 | Combined Vehicle Inertial Sensor Signal (Lat/Long Rate)

#### X206

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PU | 293 | Rear Defog Element Supply Voltage
2 | -- | -- | Not Used
3 | L-GN | 24 | Backup Lamp Supply Voltage
4 | -- | -- | Not Used
5 | -- | -- | Not Used
6 | L-BU | 1937 | Fuel Level Signal (Secondary)
7 | BN/WH | 309 | Lamp Supply Voltage
8 | -- | -- | Not Used
9 | -- | -- | Not Used
10 | -- | -- | Not Used
11 | -- | -- | Not Used
12 | PU | 709 | Left Park Lamp Supply Voltage
13 | PK | 339 | Ignition 1 Voltage
14 | -- | -- | Not Used
15 | -- | -- | Not Used
16 | -- | -- | Not Used
17 | BN/BK | 884 | Left Rear Wheel Speed Sensor Signal
18 | GY | 7128 | Right Rear Wheel Speed Sensor Supply Voltage
19 | BN/YE | 452 | Low Reference
20 | GY | 5600 | Discriminating Sensor - Low Reference
21 | YE | 354 | Discriminating Sensor - Signal
22 | D-GN/WH | 1317 | Fog Lamp Relay Control
23 | BN/WH | 2086 | Yaw Rate Sensor Test Control
24 | -- | -- | Not Used
25 | -- | -- | Not Used
26 | -- | -- | Not Used
27 | -- | -- | Not Used
28 | OG/BK | 540 | Battery Positive Voltage
29 | -- | -- | Not Used
30 | -- | -- | Not Used
31 | GY | 7127 | Left Rear Wheel Speed Sensor Supply Voltage
32 | BN | 882 | Right Rear Wheel Speed Sensor Signal
33 | PU | 1589 | Fuel Level Sensor Signal (Primary)
34 | D-GN | 1409 | Discriminating Sensor - Signal
35 | BN/YE | 5045 | Discriminating Sensor - Low Reference
36 | D-GN | 2087 | Steering Wheel Position Sensor 5-V Reference
37 | L-GN/BK | 5352 | Yaw Rate Sensor Test Control
38 | PU/WH | 1699 | Combined Vehicle Inertial Sensor Signal (Lat/Long Rate)

#### X207

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | RD/YE | 542 | Battery Positive Voltage
2 | -- | -- | Not Used

#### X207

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | RD/YE | 542 | Battery Positive Voltage
2 | -- | -- | Not Used

#### X210

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/YE | 6109 | Clutch Position Sensor Reference
2 | -- | -- | Not Used
3 | YE | 6111 | Clutch Position Sensor Signal
4 | BN/YE | 6110 | Clutch Position Sensor Return

#### X210

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/YE | 6109 | Clutch Position Sensor Reference
2 | -- | -- | Not Used
3 | YE | 6111 | Clutch Position Sensor Signal
4 | BN/YE | 6110 | Clutch Position Sensor Return

#### X212

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | -- | -- | Not Used
3 | BU | 7043 | Microphone Signal (+)
4 | L-BU | 20 | Stop Lamp Supply Voltage
5 | -- | -- | Not Used
6 | PK/BK | 7044 | Microphone Return
7 | PU | 328 | Interior Lamp Switch Signal
8 | PK/BK | 1597 | Courtesy Lamps Switch On Signal
9 | -- | -- | Not Used
10 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
11 | BK | 850 | Ground
12 | -- | -- | Not Used
13 | OG | 1732 | Courtesy Lamps Supply Voltage
14 | BK | 851 | Ground
15 | YE | 443 | Accessory Voltage
16 | OG/WH | 1840 | Battery Positive Voltage
17 | -- | -- | Not Used
18 | -- | -- | Not Used

#### X212

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | -- | -- | Not Used
2 | -- | -- | Not Used
3 | GY/BK | 7043 | Microphone Signal (+)
4 | -- | -- | Not Used
5 | -- | -- | Not Used
6 | PK/BK | 7044 | Microphone Return
7 | PU | 328 | Interior Lamp Switch Signal
8 | RD/BK | 1597 | Courtesy Lamps Switch On Signal
9 | -- | -- | Not Used
10 | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
11 | -- | -- | Not Used
12 | -- | -- | Not Used
13 | -- | -- | Not Used
14 | BK/WH | 851 | Ground
15 | -- | -- | Not Used
16 | OG/WH | 1840 | Battery Positive Voltage
17 | -- | -- | Not Used
18 | -- | -- | Not Used

#### X223

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 1050 | Ground

#### X223

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 1050 | Ground

#### X227

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN | 2501 | High Speed Gmlan Serial Data Bus -
2 | BN | 2501 | High Speed Gmlan Serial Data Bus -
3 | BN/BK | 2500 | High Speed Gmlan Serial Data Bus +
4 | BN/BK | 2500 | High Speed Gmlan Serial Data Bus +
5 | L-BU | 5986 | Communication Enable Relay Supply Voltage
6 | BK/BU | 2088 | Steering Wheel Position Sensor Low Reference

#### X227

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PU | 2501 | High Speed Gmlan Serial Data Bus -
2 | D-BU | 2501 | High Speed Gmlan Serial Data Bus -
3 | GY | 2500 | High Speed Gmlan Serial Data Bus +
4 | BN/BK | 2500 | High Speed Gmlan Serial Data Bus +
5 | L-GN | 5986 | Communication Enable Relay Supply Voltage
6 | OG | 2088 | Steering Wheel Position Sensor Low Reference

#### X241

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | D-GN | 5060 | Low Speed GMLAN Serial Data
2 | RD/WH | 1840 | Battery Positive Voltage
3 | BK | 1450 | Ground
4 | -- | -- | Not Used

#### X241

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | D-GN | 5060 | Low Speed GMLAN Serial Data
2 | OG/WH | 1840 | Battery Positive Voltage
3 | BK | 1450 | Ground
4 | -- | -- | Not Used

#### X253

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
A1 | PK | 3022 | Steering Wheel Module - Stage2 - Low Control
A2 | WH | 3023 | Steering Wheel Module - Stage2 - High Control
B1 | BN | 3020 | Steering Wheel Module - Stage1 - Low Control
B2 | BN/RD | 3021 | Steering Wheel Module - Stage1 - High Control

#### X253

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
A1 | PK | 3022 | Steering Wheel Module - Stage2 - Low Control
A2 | WH | 3023 | Steering Wheel Module - Stage2 - High Control
B1 | BN | 3020 | Steering Wheel Module - Stage1 - Low Control
B2 | BN/RD | 3021 | Steering Wheel Module - Stage1 - High Control

#### X254

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
A1 | PU | 3026 | I/P Module - Stage 2 - Low Control
A2 | D-GN | 3027 | I/P Module - Stage 2 - High Control
B1 | BU | 3024 | I/P Module - Stage 1 - Low Control
B2 | YE | 3025 | I/P Module - Stage 1 - High Control

#### X254

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
A1 | PU | 3026 | I/P Module - Stage 2 - Low Control
A2 | D-GN | 3027 | I/P Module - Stage 2 - High Control
B1 | BU | 3024 | I/P Module - Stage 1 - Low Control
B2 | YE | 3025 | I/P Module - Stage 1 - High Control

#### X303

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | WH/BU | 7391 | Non-Memory Mirror: Right Mirror Motor Up Control
2 | GY/BK | 745 | Right Front Door Ajar Switch Signal
3 | -- | -- | Not Used
4 | BN/RD | 694 | Driver Door Lock Actuator Unlock Control
5 | OG/WH | 881 | Non-Memory Mirror: Right Mirror Motor Right Control
6 | L-GN/BK | 200 | Right Front Speaker Output (+)
7 | BK | 1350 | &AXC Ground
BK | 1350 | -AXC: Ground
8 | BU/WH | 666 | Power Window Motor Right Front Up Control
9 | PK/BK | 780 | Driver Door Lock Switch Lock Signal
10 | GN/WH | 295 | Door Lock Actuator Lock Control
11 | PU/WH | 889 | Non-Memory Mirror: Right Mirror Motor Down Control
12 | D-GN | 117 | Right Front Speaker Output (-)
13 | -- | -- | Not Used
14 | BN | 667 | Power Window Motor Right Front Down Control
15 | PK | 781 | Driver Door Lock Switch Unlock Signal
16 | -- | -- | Not Used

#### X303

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | WH/BU | 7391 | Non-Memory Mirror: Right Mirror Motor Up Control
2 | GY/BK | 745 | Right Front Door Ajar Switch Signal
3 | -- | -- | Not Used
4 | BN/RD | 694 | Driver Door Lock Actuator Unlock Control
5 | OG/WH | 881 | Non-Memory Mirror: Right Mirror Motor Right Control
6 | L-GN/BK | 200 | Right Front Speaker Output (+)
7 | BK | 1350 | &AXC Ground
BK | 1350 | -AXC: Ground
8 | BU/WH | 666 | Power Window Motor Right Front Up Control
9 | PK/BK | 780 | Driver Door Lock Switch Lock Signal
10 | GN/WH | 295 | Door Lock Actuator Lock Control
11 | PU/WH | 889 | Non-Memory Mirror: Right Mirror Motor Down Control
12 | D-GN | 117 | Right Front Speaker Output (-)
13 | -- | -- | Not Used
14 | BN | 667 | Power Window Motor Right Front Down Control
15 | PK | 781 | Driver Door Lock Switch Unlock Signal
16 | -- | -- | Not Used

#### X304

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | WH/BU | 7391 | Non-Memory Mirror: Left Mirror Motor Up Control
2 | BN/WH | 746 | Left Front Door Ajar Switch Signal
3 | -- | -- | Not Used
4 | BN/RD | 294 | Driver Door Lock Actuator Unlock Control
5 | WH/BK | 81 | Non-Memory Mirror: Left Mirror Motor Right Control
6 | BN | 201 | Left Front Speaker Output (+)
7 | BK | 2050 | &AXC: Ground
BK | 20205 | -AXC: Ground
8 | D-BU | 164 | Power Window Motor Left Front Up Control
9 | PK/BK | -- | Not Used
10 | GN/WH | 295 | Door Lock Actuator Lock Control
11 | L-GN/BK | 89 | Non-Memory Mirror: Left Mirror Motor Down Control
12 | GY | 118 | Left Front Speaker Output (-)
13 | -- | -- | Not Used
14 | BN/OG | 165 | Power Window Motor Left Front Down Control
15 | PK | -- | Not Used
16 | -- | -- | Not Used

#### X304

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | WH/BU | 7391 | Non-Memory Mirror: Left Mirror Motor Up Control
2 | BN/WH | 746 | Left Front Door Ajar Switch Signal
3 | -- | -- | Not Used
4 | BN/RD | 294 | Driver Door Lock Actuator Unlock Control
5 | WH/BK | 81 | Non-Memory Mirror: Left Mirror Motor Right Control
6 | BN | 201 | Left Front Speaker Output (+)
7 | BK | 2050 | &AXC: Ground
BK | 20205 | -AXC: Ground
8 | D-BU | 164 | Power Window Motor Left Front Up Control
9 | PK/BK | -- | Not Used
10 | GN/WH | 295 | Door Lock Actuator Lock Control
11 | L-GN/BK | 89 | Non-Memory Mirror: Left Mirror Motor Down Control
12 | GY | 118 | Left Front Speaker Output (-)
13 | -- | -- | Not Used
14 | BN/OG | 165 | Power Window Motor Left Front Down Control
15 | PK | -- | Not Used
16 | -- | -- | Not Used

#### X305

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 1350 | Ground
2 | GY | 120 | Fuel Pump Supply Voltage
3 | L-BU | 1937 | Fuel Level Sensor Signal (Secondary)
4 | BN/YE | 452 | Low Reference
5 | PU | 1589 | Fuel Level Sensor Signal (Primary)

#### X305

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK | 1350 | Ground
2 | GY | 120 | Fuel Pump Supply Voltage
3 | L-BU | 1937 | Fuel Level Sensor Signal (Secondary)
4 | BN/YE | 452 | Low Reference
5 | PU | 1589 | Fuel Level Sensor Signal (Primary)

#### X309

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/BK | 233 | Park Brake Switch Signal
2 | BN/YE | 143 | Accessory Voltage
3 | -- | -- | Not Used
4 | GY | 8 | Instrument Panel Lamp Supply Voltage
5 | BK | 2050 | Ground
6 | -- | -- | Not Used

#### X309

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG/BK | 233 | Park Brake Switch Signal
2 | BN/YE | 143 | Accessory Voltage
3 | -- | -- | Not Used
4 | GY | 8 | Instrument Panel Lamp Supply Voltage
5 | BK | 2050 | Ground
6 | -- | -- | Not Used

#### X311

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | RD | 1140 | Battery Positive Voltage
2 | BK | 350 | Ground
3 | BK/WH | 238 | Seat Belt Switch - Left Front
4 | D-BU | 1363 | Seat Belt Switch - Left - Low Reference

#### X311

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | OG | 1140 | Battery Positive Voltage
2 | BK | 2050 | Ground
3 | BK/WH | 238 | Seat Belt Switch - Left Front
4 | D-BU | 1363 | Seat Belt Switch - Left - Low Reference

#### X315

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | PK/BU | 5055 | Seat Position Sensor- Right Front - Signal
2 | PU/WH | 1363 | Seat Belt Switch - Right Front - Low Reference

#### X315

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | L-GN | 5055 | Seat Position Sensor- Right Front - Signal
2 | D-BU | 1363 | Seat Belt Switch - Right Front - Low Reference

#### X328

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
C | GY | 6001 | Radio Antenna Post
S | BARE | 6015 | Radio Antenna Shield

#### X328

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
C | GY | 6001 | Radio Antenna Post
S | BARE | 615 | Radio Antenna Shield

#### X355

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | L-GN | 2116 | Seat Belt Pretensioner - RT High Control
2 | OG | 2117 | Seat Belt Pretensioner - Low Control

#### X355

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | L-GN | 316 | Seat Belt Pretensioner - High Control
2 | OG | 2117 | Seat Belt Pretensioner - Low Control

#### X356

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK/WH | 2118 | Seat Belt Pretensioner - High Control
2 | OG/BK | 2119 | Seat Belt Pretensioner - Low Control

#### X356

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BK/WH | 2118 | Seat Belt Pretensioner - High Control
2 | OG/BK | 2119 | Seat Belt Pretensioner - Low Control

#### X360

Connector Part Information | Male
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN/BK | 884 | Left Rear Wheel Speed Sensor Signal
2 | BN | 882 | Right Rear Wheel Speed Sensor Signal
3 | GY | 7127 | Left Rear Wheel Speed Sensor Supply Voltage
4 | GY | 7128 | Right Rear Wheel Speed Sensor Supply Voltage

#### X360

Connector Part Information | Female
--- | ---
Pin | Wire Colour | Circuit Number | Function
1 | BN/BK | 884 | Left Rear Wheel Speed Sensor Signal
2 | BN | 882 | Right Rear Wheel Speed Sensor Signal
3 | GY | 7127 | Left Rear Wheel Speed Sensor Supply Voltage
4 | GY | 7128 | Right Rear Wheel Speed Sensor Supply Voltage