For 1990-2009 cars

### Handling Procedure

1. Do not carry a seat belt pretensioner by it's wiring harness lead.
2. Do not apply power to a pretensioner except as specified.
3. Do not attempt to make any repairs to the pretensioner assembly. A damaged or defective component must be replaced.
4. Do not weld, solder, braze, hammer, machine drill, or otherwise heat any SIR component.

### Deployment Procedure - (In Vehicle)

Refer to Inflator Module Handling and Scrapping .

### Deployment Procedure - (Out Of Vehicle)

Refer to TAS (Technical Assistant Service) for further instructions.