For 1990-2009 cars

#### Tools Required

• |
- J 28467-B Universal Engine Support Fixture

• |
- J 41803 Engine Support Fixture

• |
- J 41798 Engine Lift Bracket

### Removal Procedure

1. Remove the engine cover. Refer to Engine Cover Replacement .
2. Remove the Oil Level Indicator and Tube. Refer to Oil Level Indicator and Tube Replacement .

Caution: Refer to Vehicle Lifting Caution in the Preface section.

3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
4. Remove the engine splash shield. Refer to Engine Splash Shield Replacement .
5. Remove the lower engine mount to front subframe retaining nut (1) from both engine mounts.
6. Lower the vehicle.
7. Remove the upper right side engine mount to engine mount bracket retaining nut 1).
8. Position the J 41798 (1) on the cylinder head (3).

Notice: Refer to Fastener Notice in the Preface section.

9. Install the J 41798 to cylinder head retaining bolts (2).

Tighten
Tighten the bolts to 50 N·m (36 lb ft).

Important: When lifting the engine assembly, observe the clearance between the rear of the engine assembly and the dash panel.

10. Install J 41803 and J 28467-B and raise the engine assembly until the right side engine mount bracket (1) is clear of the right side engine mount retaining stud (2).

Important: DO NOT bend or distort the right side engine mount heat shield (4).

11. Remove the right side engine mount assembly (3).

### Installation Procedure

Important: DO NOT bend or distort the right side engine mount heat shield (4).

1. Install the right side engine mount assembly (3).
2. Lower the engine assembly until the right side engine mount retaining stud (2) is installed through the right side engine mount bracket (1).
3. Remove J 41803 , J 28467-B and J 41798 from the engine.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the upper right side engine mount to engine mount bracket retaining nut (1).

Tighten
Tighten the nut to 80 N·m (59 lb ft).

Caution: Refer to Vehicle Lifting Caution in the Preface section.

5. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .

Notice: Refer to Fastener Notice in the Preface section.

6. Install the lower engine mount to front subframe retaining nut (1) on both engine mounts.

Tighten
Tighten the nut to 80 N·m (59 lb ft).

7. Install the engine splash shield. Refer to Engine Splash Shield Replacement .
8. Lower the vehicle.
9. Install the Oil Level Indicator and Tube. Refer to Oil Level Indicator and Tube Replacement .
10. Install the engine cover. Refer to Engine Cover Replacement .