For 1990-2009 cars

### IPC Replacement

Important: The original odometer reading, together with other important vehicle parameters, must be programmed into the replacement instrument cluster. If a replacement cluster has been fitted to a vehicle it will require programming, the vehicle type must be selected followed by the country and then the engine type. The engine type is required only for some countries and this is highlighted below.

If the instrument panel cluster (IPC) is replaced, the following procedures must be performed in the order shown:

1. Odometer reprogramming.

Important: The IPC variant configuration must be correct or the performance of the EBCM will be reduced.

2. Variant configuration.
3. IPC reprogramming - Refer to Service Programming System (SPS) .

### Program Odometer

Important: It is only possible to reset the odometer reading if no more than 100 km has been registered on the odometer. It is essential to enter the correct odometer value, as the programming of the odometer can only be performed once.

Important: Programming the odometer is prohibited without TIS approval. Refer to Obtaining TIS Approval for more information.

1. Install a diagnostic scan tool.
2. Select Body.
3. Select IPC (Instrument Panel Cluster).
4. Select Programming.
5. Select the Program Odometer procedure and follow the directions displayed on the screen.
6. Obtain TIS approval then repeat steps 1-5.

### Program Variant Configuration

This option allows you to reconfigure the instrument panel cluster (IPC) from the default factory settings.

Important: Regular production options (RPOs) are located on the vehicle security card.

Prior to removal use a scan tool to identify the existing RPOs that are programmed into the IPC.

The following options are available:

1. Car Body Style.

• | 4 Door Short Wheel Base Sedan.

• | 4 Door Long Wheel Base Sedan.

2. Engine Type.

• | 3.6 L V6 (LE0)

• | 3.6 L V6 (LY7)

• | 3.6 L V6 LPG (LW2)

• | 6.0 L V8 (L76/L98)

• | 6.0 L V8 HSV (LS2)

3. Transmission Type.

• | 6 Speed Manual (D173) MV5

• | 6 Speed Manual (T56) M10

• | 4 Speed Automatic RWD (4L60E) M30

• | 4 Speed Automatic RWD (4L65E) M32

• | 5 Speed Automatic RWD (5L40E) M82

• | 6 Speed Automatic RWD (6L80E) MYC

4. Suspension Type.

• | Unknown

• | Standard FE1

• | Sports FE2

• | Country FR1

5. Country.

• | Australia (B13)

• | New Zealand (E13)

• | Middle East (E05)

• | Brazil (B08)

• | South Africa (B02)

• | Indonesia (B00)

6. Tyre Pressure Monitoring.

• | Not Fitted

• | Fitted

7. Police Mode.

• | Disabled

• | Enabled

8. Navigation.

• | Not Fitted

• | TBT Nav (UY4)

• | Full Nav (UV9)

9. Fleet Telematics (U86).

• | Not Fitted

• | Fitted

10. LPG.

• | Not Fitted

• | Fitted

11. AHL (Automatic Headlamp Levelling).

• | Not Fitted

• | Fitted

#### Programming

1. Install a diagnostic scan tool.
2. Select Body.
3. Select IPC (Instrument Panel Cluster).
4. Select Programming.
5. Select the Program Variant Configuration procedure and follow the directions displayed on the screen.
6. Obtain TIS approval then repeat steps 1-5.

Perform the Diagnostic Repair Verification after completing the proceeding procedures.