For 1990-2009 cars

### Removal Procedure

Important: The front floor console front cover (1) is retained by clips.

1. Grasp the front floor console front cover (1) at (A) and pull upwards to disengage the retaining clips from the floor console (2).
2. Disconnect the window and exterior mirror switch electrical connector (2).
3. Disconnect the Traction Control/ESP and Power switch (if fitted) electrical connectors (3).
4. Remove the front floor console front cover (1).

### Installation Procedure

1. Connect the Traction Control/ESP and Power switch (if fitted) electrical connectors (3).
2. Connect the window and exterior mirror switch electrical connectors (2).
3. Install the front floor console front cover (1).

Important: The front floor console front cover (1) is retained by clips.

4. Install the front floor console front cover (1) and push downwards at (A) to engage the retaining clips to the floor console (2).
5. Test all switches for correct operation.