For 1990-2009 cars

### Removal Procedure

1. Lift the fluid level indicator handle lock up.
2. Remove the fluid level indicator.
3. Remove the bolt attaching the fill tube to the cylinder head.
4. Remove the fill tube and seal from the transmission.

### Installation Procedure

1. Insert the seal into the automatic transmission case hole.
2. Install the fill tube to the transmission.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the transmission bolt attaching the fill tube to the cylinder head.

Tighten
Tighten the fill tube bolt to 30 N·m (22 lb ft).

4. Check the transmission fluid level.
5. Fill the transmission to the proper level with DEXRON® VI transmission fluid. Refer to Transmission Fluid Check.
6. Push the fluid level indicator handle lock down.