For 1990-2009 cars

#### Tools Required

J 35667-A Cylinder Head Leakdown Tester, or equivalent

Important: A leakage test may be performed in order to measure cylinder/combustion chamber leakage. High cylinder leakage may indicate one or more of the following conditions:

• | Worn or burnt valves.

• | Broken valve springs.

• | Stuck valve lifters.

• | Incorrect valve lash.

• | Damaged piston.

• | Worn piston rings.

• | Worn or scored cylinder bore.

• | Damaged cylinder head gasket.

• | Cracked or damaged cylinder head.

• | Cracked or damaged engine block.

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery ground negative cable.
2. Remove the spark plugs. Refer to Spark Plug Inspection.
3. Rotate the crankshaft to place the piston in the cylinder being tested at top dead centre (TDC) of the compression stroke.
4. Install the J 35667-A or equivalent.

Important: It may be necessary to hold the crankshaft balancer bolt to prevent the crankshaft from rotating.

5. Apply compressed air pressure to the J 35667-A and adjust according to the manufacturers instructions.
6. Record the cylinder leakage value. Cylinder leakage that exceeds 25 percent is considered above acceptable and may require component service. In above acceptable leakage situations, inspect for the following conditions:

• | Air leakage noise at the throttle body or air inlet hose that may indicate a worn or burnt intake valve or a broken valve spring.

• | Air leakage noise at the exhaust system tail-pipe that may indicate a worn or burnt exhaust valve or a broken valve spring.

• | Air leakage noise from the crankcase, oil level indicator tube, or oil fill tube that may indicate worn piston rings, a damaged piston, a worn or scored cylinder bore, a damaged engine block or a damaged cylinder head.

• | Air bubbles in the cooling system may indicate a damaged cylinder head or a damaged cylinder head gasket.

7. Perform the leakage test on the remaining cylinders and record the values.