For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the oil pan cover to oil pan retaining bolts (2).
3. Remove the cover (1).
4. Remove the gasket (3).

### Installation Procedure

1. Position the gasket (3) and cover (1) on the engine block.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the retaining bolts (2) for the cover.

Tighten
Tighten the bolts to 12 N·m (106 lb in).

3. Lower the vehicle.