For 1990-2009 cars

### Removal Procedure

#### Tools Required

• |
- J 41816 Crankshaft Balancer Remover

• |
- J 41816-2 Crankshaft End Protector

• |
- J 42386-A Flywheel Holding Tool

1. Remove the right transmission cover (1) to engine oil pan retaining bolt (2).
2. Remove the right transmission cover (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Using the two starter motor bolts (2), install the J 42386-A (1).

Tighten
Tighten the bolts to 50 N·m(37 lb ft).

Important: DO NOT discard the crankshaft balancer bolt. The balancer bolt will be used during the first pass only of the balancer installation procedure. Install a NEW crankshaft balancer bolt at second pass, during final assembly.

4. Remove the crankshaft balancer retaining bolt (1).
5. Use the J 41816 (1) and J 41816-2 (2) to remove the crankshaft balancer (3).