For 1990-2009 cars

#### Tools Required

• | DT-47721 Shift Shaft Seal Installer

• | DT-47725 Extension Housing Bearing Cup Installer

• | J 21128 Axle Pinion Oil Seal Installer

• | J 36614 Inner Pinion Bearing Installer

1. Using DT-47725 and J 36614 , install the tapered bearing race (1).
2. Apply an approved gear oil and install the tapered roller bearing (1).
3. Using J 21128 , install a NEW rear output seal (1).
4. Using DT-47721 , install a NEW shift shaft seal (1).