For 1990-2009 cars

### Removal Procedure

Important: Carefully remove the radiator grille applique from the radiator grille. Failure to do so will result in damage to the radiator grille applique.

1. Remove the radiator grille. Refer to Radiator Grille Replacement.
2. Remove the radiator grille applique to radiator grille retaining screws (1).
3. Remove the radiator grille applique by releasing the retaining clips (1).
4. Remove the radiator grille applique from the radiator grille.
5. Remove the radiator grille emblem. Refer to Radiator Grille Emblem/Nameplate Replacement.

### Installation Procedure

1. Install the radiator grille emblem. Refer to Radiator Grille Emblem/Nameplate Replacement.
2. Install the radiator grille applique to the radiator grille.
3. Apply pressure to the radiator grille applique to engage the retaining clips (1) to the radiator grille.
4. Make sure that the retaining clips are secure.

Notice: Refer to Fastener Notice in the Preface section.

5. Install the radiator grille applique to radiator grille retaining screws (1).

Tighten
Tighten the screws to 2 N·m (18 lb in).

6. Install the radiator grille. Refer to Radiator Grille Replacement.