For 1990-2009 cars

### Removal Procedure

1. Remove the push-in front door upper auxiliary weatherstrip to door retaining fasteners.

Important: Remove the weatherstrip by pulling to release retaining fasteners.

2. Remove the front door upper auxiliary weatherstrip (1) from the door (2).

### Installation Procedure

Important: Install the weatherstrip by pushing to attach retaining fasteners.

1. Install the front door upper auxiliary weatherstrip moulding (1) to the door (2).
2. Install the push-in fasteners to the door.