For 1990-2009 cars

Checks | Causes
--- | ---
Centre Support with 2-6 Low and Reverse Clutch Assembly (67) |

• | Inspect for damaged or worn output carrier outer sun gear shaft front bushing (458).

• | Inspect for damaged or worn output carrier outer sun gear shaft rear bushing (460).

• | Inspect for damaged 2-6 clutch backing plate (451). Inspect for worn splines on backing plate.

• | Inspect for damaged 2-6 clutch backing plate retaining ring (450).

• | Inspect for damaged 2-6 clutch piston assembly (457), spring (456), retaining ring (455), and centre support assembly (459).