For 1990-2009 cars

### Removal Procedure

1. Remove the radiator grille to front end module retaining bolts (1).
2. Remove the radiator grille to front end module push-in retainers (2).
3. Carefully pry the radiator grille retaining tabs (1) from the upper edge of the front bumper fascia.
4. Remove the radiator grille from the front bumper fascia.

### Installation Procedure

1. Install the radiator grille to the front bumper fascia.
2. Firmly press the radiator grille retaining tabs (1) into the upper edge of the front bumper fascia.
3. Install the radiator grille to front end module push-in retainers (2).

Notice: Refer to Fastener Notice in the Preface section.

4. Install the radiator grille to front end module retaining bolts (1).

Tighten
Tighten the bolts to 4.5 N·m (39 lb in).