For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the front bumper fascia support bracket to front end module retaining bolts (1).
3. Remove the horn wiring harness clip from the front bumper fascia support bracket.
4. Remove the front bumper fascia support bracket from the vehicle.

### Installation Procedure

1. Install the front bumper fascia support bracket to the front end module.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front bumper fascia support bracket to front end module retaining bolts (1).

Tighten
Tighten the bolts to 4.5 N·m (39 lb in).

3. Install the horn wiring harness clip to front bumper fascia support bracket.
4. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .