For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provide an overview of each diagnostic category.

### DTC Descriptors

DTC P0601: Control Module Read Only Memory (ROM)
DTC P0602: Control Module Not Programmed
DTC P0603: Control Module Long Term Memory Reset
DTC P0604: Control Module Random Access Memory (RAM)
DTC P0606: Control Module Internal Performance
DTC P0607: Control Module Performance
DTC P060D: Control Module Accelerator Pedal Position (APP) System Performance
DTC P062F: Control Module Long Term Memory Performance
DTC P2610: Control Module Ignition Off Timer Performance

### Description

This diagnostic applies to internal microprocessor integrity conditions within the engine control module (ECM) and the throttle actuator control (TAC) system. This diagnostic also addresses if the ECM is not programmed.

The ECM monitors its ability to read and write to the memory. It also monitors a timing function. The ECM and the TAC processors are used to monitor the TAC system data. Both processors monitor the other processors data to verify that the indicated APP calculation is correct. The ECM performs an intrusive test in order to confirm that the APP signals are not shorted together. The ECM accomplishes this by pulling the APP sensor 2 low momentarily and looking for sensor 1 to also be pulled low.

### Conditions for Running the DTC

#### P0601

• | The ignition switch is in Run or Crank.

• | DTC P0601 runs continuously when the above condition is met.

#### P0602

• | The ignition switch is in Run or Crank.

• | DTC P0602 runs once per ignition cycle.

#### P0603

• | The ignition switch is in Run or Crank.

• | DTC P0603 runs once per ignition cycle.

#### P0604

• | The ignition switch is in Run or Crank.

• | DTC P0604 runs continuously when the above condition is met.

#### P0606

• | The ignition switch is in the Unlock/Accessory, Run, or Crank positions.

• | The system voltage is more than 5.23 volts.

• | DTC P0606 runs continuously when the above conditions are met.

#### P0607

• | The ignition switch is in Unlock, Accessory, Run or Crank.

• | The system voltage is more than 5.23 volts.

• | DTCs P0601, P0602, P0603, P0604, P0606, P062F, P0641, P0651, P2610 are not set

• | DTC P0607 runs continuously when the above conditions are met.

#### P060D

• | DTC P0606 is not set.

• | The ignition switch is in the Unlock, Accessory, Run, or Crank position.

• | The system voltage is more than 5.23 volts.

• | DTC P060D runs continuously when the above conditions are met.

#### P062F

• | The ignition is ON.

• | DTC P062F runs once per ignition cycle.

#### P2610

• | The ECM is powered down.

• | The intake air temperature is between -40 to +125°C (-40 to +257°F).

• | DTC P2610 runs once per ignition cycle.

### Conditions for Setting the DTC

The ECM detects an internal failure or incomplete programming for more than 10 seconds.

### Actions Taken When the DTC Sets

• | DTCs P0601, P0602, P0603, P0604, P0606, P060D, and P062F are Type A DTCs.

• | DTC P0607 is a Type C DTC.

• | DTC P2610 is a Type B DTC.

### Conditions for Clearing the MIL/DTC

• | DTCs P0601, P0602, P0603, P0604, P0606, P060D, and P062F are Type A DTCs.

• | DTC P0607 is a Type C DTC.

• | DTC P2610 is a Type B DTC.

### Reference Information

#### DTC Type Reference

Powertrain Diagnostic Trouble Code (DTC) Type Definitions

### Circuit/System Testing

1. Observe the DTCs with the scan tool.

⇒ | If DTC P0602 is set, attempt to program the ECM before replacing the ECM. Refer to Service Programming System (SPS).

⇒ | If DTC P0602 resets, replace the ECM.

Important: An intermittent or momentary, less than 1 second, loss of system voltage during throttle tip-in may set DTC P060D.

2. Test the voltage and ground inputs to the ECM for the following:

• | A short

• | An open

• | High resistance

⇒ | If all circuits test normal, replace the ECM.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

Control Module References for ECM replacement, programming and setup