For 1990-2009 cars

### Removal Procedure

1. Remove the cargo liner to cargo tie down plate retaining bolts (2).
2. Remove the cargo tie down plate (1) from the cargo liner (3).

### Installation Procedure

1. Install the tie down bracket (1) to the cargo liner (3).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the cargo area to tie down bracket retaining bolts (2).

Tighten
Tighten the bolts to 22 N·m (16 lb ft).