For 1990-2009 cars

#### Tools Required

J 38836 Bushing Installer and Clutch Arbor

Important: Make sure that the crankshaft rear oil gallery plug (1) is not a loose fit, damaged or leaking.

Important: The correct depth (a) for the oil gallery plug is 31.2 to 31.6 mm.

1. Apply sealant LOCTITE R 242 and install it to the correct depth, If replacing the oil gallery plug (1).

Important: Use a 5/8 inch flat washer (2) against the tool to support the bearing races.

Important: When installed correctly the bearing should be flush with the crankshaft counter-bore.

2. Install the clutch pilot bearing (3) to the rear of the crankshaft, using J 38836 (1).