For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Reverse Lamp Switch | 27 N·m | 20 lb ft
Concentric Slave Cylinder Retaining Bolt | 12 N·m | 108 lb in
Drive Flange Retaining Nut | 135 N·m | 100 lb ft
Reverse Lockout Assembly Retaining Bolt | 18 N·m | 13 lb ft
Reverse Lockout Solenoid | 40 N·m | 30 lb ft
Shift Rail Roller Detent Bolt | 20 N·m | 14 lb ft
Shift Guide Plate Retaining Bolt | 22 N·m | 16 lb ft
Transmission Retaining Bolt | 48 N·m | 35 lb ft
Transmission Fill Plug | 28 N·m | 13 lb ft
Transmission Drain Plug | 28 N·m | 13 lb ft
Transmission Mount To Transmission Case Retaining Bolts | 60 N·m | 44 lb ft
Adapter Plate Plug | 27 N·m | 20 lb ft
Adapter Plate To Transmission Case Retaining Bolts | 48 N·m | 36 lb ft
Shift Turrett Retaining Bolts | 20 N·m | 15 lb ft
Extension Housing Plug | 27 N·m | 20 lb ft
Extension Housing To Transmission Case Retaining Bolts | 48 N·m | 36 lb ft
Neutral Return Cam Spring Retaining Bolt | 25 N·m | 18 lb ft
Reverse Idler Shaft Bracket Retaining Bolts | 25 N·m | 18 lb ft
Shift Detent Assembly | 40 N·m | 30 lb ft
Shift Interlock Retaining Bolts | 27 N·m | 20 lb ft
Reverse Lamp Switch Bolt | 4 N·m | 6 lb ft
CSC Pipe Bracket Bolt | 4 N·m | 6 lb ft
Bell Housing to Adaption Bolt | 48 N·m | 36 lb ft