For 1990-2009 cars

Notice: DO NOT use cooling system seal tabs, or similar compounds, unless otherwise instructed. The use of cooling system seal tabs, or similar compounds, may restrict coolant flow through the passages of the cooling system or the engine components. Restricted coolant flow may cause engine overheating and/or damage to the cooling system or the engine components/assembly.

Important: Ensure all mating surfaces are clean and free of grease.

1. Insert two retaining bolts (1) at each end of the pump, place the new gasket of the bolts and use this as a guide to install the pump.

Notice: Refer to Fastener Notice in the Preface section.

2. Install and tighten the remaining bolts.

Tighten
Tighten the water pump pulley bolts to 25 N·m (18 lb ft).