For 1990-2009 cars

Important: DO NOT use the throttle body gasket again. Install a NEW gasket during assembly.

Important: Align the locating tab of the gasket with the notch in the manifold.

1. Install the throttle body gasket (2).
2. Install the throttle body (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the throttle body to intake manifold retaining bolts (3).

Tighten
Tighten the bolts to 10 N·m (89 lb in).