For 1990-2009 cars

### Removal Procedure

#### Type A

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front air deflector. Refer to Front Air Deflector Replacement.

Important: Carefully pry the front fog lamp cover from the front bumper fascia

3. Disengage the front fog lamp cover retaining tabs (1) from the front bumper fascia.
4. Remove the front fog lamp cover from the vehicle.

### Removal Procedure

#### Type B

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front air deflector. Refer to Front Air Deflector Replacement.

Important: Carefully pry the front fog lamp cover from the front bumper fascia

3. Disengage the front fog lamp cover retaining tabs (1) from the front bumper fascia.
4. Remove the front fog lamp cover from the vehicle.

### Installation Procedure

#### Type A

1. Install the front fog lamp cover to the front bumper fascia.
2. Firmly press the front fog lamp cover retaining tabs (1) into the front bumper fascia.
3. Install the front air deflector. Refer to Front Air Deflector Replacement.
4. Lower the vehicle.

### Installation Procedure

#### Type B

1. Install the front fog lamp cover to the front bumper fascia.
2. Firmly press the front fog lamp cover retaining tabs (1) into the front bumper fascia.
3. Install the front air deflector. Refer to Front Air Deflector Replacement.
4. Lower the vehicle.