For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery ground cable from the battery. Refer to Battery Negative Cable Disconnection and Connection .

Caution: Refer to SIR Caution in the Preface section.

2. Disable the SIR system. Refer to SIR Disabling and Enabling in SIR.
3. Remove the front seat. Refer to Front Seat Replacement - Bucket .
4. Remove the front seat adjuster. Refer to Front Seat Adjuster Replacement .
5. Remove seat-back frame assembly. Refer to Front Seat Back Frame Replacement .
6. Disengage the front and side J-strips (2) away from the seat adjuster (3).
7. Remove the front seat cushion (1).

### Installation Procedure

1. Install the front seat cushion (1) onto the front seat adjuster (3).
2. Engage the front and side J-strips (2) onto the seat adjuster (3).
3. Install seat-back frame assembly. Refer to Front Seat Back Frame Replacement .
4. Install the front seat. Refer to Front Seat Replacement - Bucket .

Caution: Refer to SIR Caution in the Preface section.

5. Enable the SIR system. Refer to SIR Disabling and Enabling in SIR.
6. Connect the battery ground cable to the battery. Refer to Battery Negative Cable Disconnection and Connection .
7. Test the seat for correct mechanical and electrical operation.