For 1990-2009 cars

### Removal Procedure

1. Remove the oil filler cap.
2. Remove the engine cover. Refer to Engine Cover Replacement.
3. Disconnect the manifold absolute pressure (MAP) sensor wiring harness connector (1).
4. Disengage the MAP sensor (2) to MAP sensor retaining clip.
5. Remove the MAP sensor (1) from the intake manifold.
6. Check the MAP sensor seal (2) for deterioration, replace if necessary.

### Installation Procedure

1. Install the MAP sensor (1) to the intake manifold.
2. Make sure that the MAP sensor (2) is engaged into the MAP sensor retaining clip.
3. Connect the MAP sensor wiring harness connector (1) to the MAP sensor.
4. If re-programming is required. Refer to Control Module References .
5. Install the engine cover. Refer to Engine Cover Replacement .
6. Install the oil filler cap.