For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Inlet Assembly To HVAC Module Assembly Retaining Screws | 9 N·m | 80 lb in
Air Outlet Duct to Instrument Panel (I/P) Upper Trim Pad Retaining Screws | 2 N·m | 18 lb in
Automatic Transmission Cooler Pipe Clamp to A/C Bracket Retaining Bolt | 23 N·m | 17 lb ft
Blower Motor to Blower Assembly Retaining Screws | 1.2 N·m | 11 lb in
Blower Scroll to HVAC Case Retaining Screws | 1 N·m | 9 lb in
Compressor Mounting Bracket to Cylinder Block Retaining Bolts 3.6L | 58 N·m | 43 lb ft
Compressor Mounting Bracket to Cylinder Block Retaining Bolts 6.0L | 58 N·m | 43 lb ft
Compressor to Compressor Mounting Bracket Retaining Bolts 3.6L | 22 N·m | 16 lb ft
Compressor to Compressor Mounting Bracket Retaining Bolts 6.0L | 22 N·m | 16 lb ft
Compressor Drive Belt Tensioner to Compressor Mounting Bracket Retaining Bolt 3.6L | 58 N·m | 43 lb ft
Compressor Drive Belt Tensioner to Compressor Mounting Bracket Retaining Bolt 6.0L | 58 N·m | 43 lb ft
Condenser Discharge Hose Bolt | 22 N·m | 16 lb ft
Discharge Pipe to Condenser Retaining Nut | 22 N·m | 16 lb ft
Condenser Mounting Bolts | 11 N·m | 97 lb in
Floor Air Outlet Duct to I/P Retaining Screws | 2 N·m | 18 lb in
Heater Core Pipe Locating Plate To HVAC Module Assembly Retaining Screw | 1 N·m | 9 lb in
Heater Core Retaining Plate to HVAC Module Assembly Retaining Screw | 1 N·m | 9 lb in
HVAC Module Assembly to Bulkhead Retaining Bolts | 7 N·m | 62 lb in
HVAC Module Assembly to I/P Carrier Retaining Screws | 9 N·m | 80 lb in
I/P Center Air Outlet Deflector to I/P Upper Trim Panel Retaining Screws | 2 N·m | 18 lb in
Left Engine Cover Mounting Bracket to Cylinder Head Retaining Bolt | 35 N·m | 26 lb in
Liquid Pipe Bracket Screw | 22 N·m | 16 lb ft
Rear Air Outlet Duct Nut | 1 N·m | 9 lb in
Refrigerant Pressure Sensor | 6 N·m | 53 lb in
Remote Battery Positive Post to Wiring Harness Retaining Bolt | 15 N·m | 11 lb ft
Suction/Discharge Pipe to Compressor Retaining Bolt | 22 N·m | 16 lb in
Suction Pipe/Liquid Pipe Pad to TX Valve Retaining Nut | 22 N·m | 16 lb ft
Suction Pipe/Liquid Pipe Retaining Clip to Left Front Chassis Rail Retaining Bolt | 22 N·m | 16 lb ft
Suction Pipe Upper to Suction Pipe Lower Retaining Nut | 22 N·m | 16 lb in
TX Valve Retaining Bolts | 4 N·m | 35 lb ft