For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### DTC Descriptors

DTC P0133: HO2S Slow Response Bank 1 Sensor 1
DTC P0134: HO2S Circuit Insufficient Activity Bank 1 Sensor 1
DTC P0140: HO2S Circuit Insufficient Activity Bank 1 Sensor 2
DTC P1133: HO2S Insufficient Switching Bank 1 Sensor 1
DTC P2270: HO2S Signal Stuck Lean Bank 1 Sensor 2
DTC P2271: HO2S Signal Stuck Rich Bank 1 Sensor 2

### Diagnostic Fault Information

Circuit | Short to Ground | High Resistance | Open | Short to Voltage | Signal Performance
--- | --- | --- | --- | --- | ---
HO2S High Signal | P0131, P0132, P0137, P0140, P0151, P0152, P0157, P0158, P1133 | P0131, P0132, P0133, P0134, P0137, P0140, P0151, P0152, P0153, P0154, P0157, P0160, P1133, P1153 | P0131, P0132, P0133, P0134, P0137, P0140, P0151, P0152, P0153, P0154, P0157, P0160, P1133, P1153 | P0132, P0134, P0138, P0140, P0152, P0154, P0158, P0160, P1133, P1153 | P0133, P0134, P0140, P0153, P0154, P0160, P1133, P1153, P2270, P2271
HO2S Low Signal | -- | P0131, P0132, P0133, P0134, P0138, P0140, P0151, P0152, P0153, P0154, P0158, P0160, P1133 | P0131, P0132, P0133, P0134, P0138, P0140, P0151, P0152, P0153, P0154, P0158, P0160, P1133, P1153 | P0134, P0138, P0140, P0154, P0158, P0160, P1133, P1153 | --

### Typical Scan Tool Data

#### HO2S Sensor 1 Voltage

Circuit | Short to Ground | Open | Short to Voltage
--- | --- | --- | ---
Parameter Normal Range: 200-800 mV
HO2S High Signal | 0 mV | Approximately 470 mV | Approximately 1,100 mV
HO2S Low Signal | 455 mV | Approximately 450 mV | Approximately 445 mV

### Circuit/System Description

Heated oxygen sensors (HO2S) are used for fuel control and post catalyst monitoring. Each HO2S compares the oxygen content of the surrounding air with the oxygen content in the exhaust stream. The HO2S must reach operating temperature to provide an accurate voltage signal. Heating elements inside the HO2S minimize the time required for the sensors to reach operating temperature. The engine control module (ECM) supplies the HO2S with a reference, or bias, voltage of about 450 mV. When the engine is first started, the ECM operates in Open Loop, ignoring the HO2S voltage signal. Once the HO2S reaches operating temperature and Closed Loop is achieved, the HO2S generates a voltage within a range of 0-1,000 mV that fluctuates above and below bias voltage. High HO2S voltage indicates a rich exhaust stream. Low HO2S voltage indicates a lean exhaust stream.

### Conditions for Running the DTC

#### P0133

• | DTCs P0068, P0101, P0102, P0103, P0106, P0107, P0108, P0112, P0113, P0116, P0117, P0118, P0120, P0121, P0122, P0123, P0128, P0201, P0202, P0203, P0204, P0205, P0206, P0207, P0208, P0220, P0222, P0223, P0442, P0443, P0446, P0449, P0455, P0496, P1516, P2101, P2119, P2135, P2176 are not set.

• | The Engine Coolant Temperature (ECT) Sensor parameter is more than 60°C (140°F).

• | The Intake Air Temperature (IAT) Sensor parameter is more than -40°C (-40°F)

• | The Ignition 1 Signal parameter is between 10-18 volts.

• | The Fuel Level Sensor parameter is more than 10 percent.

• | The Engine Run Time parameter is more than 160 seconds.

• | The Engine Speed parameter is between 1,200-3,000 RPM.

• | The Barometric (BARO) Pressure parameter is more than 70 kPa.

• | The Mass Airflow (MAF) Sensor parameter is between 20-55 g/s.

• | The Loop Status parameter is Closed.

• | The Throttle Position (TP) Indicated Angle parameter is more than 5 percent.

• | DTC P0133 runs once per drive cycle when the above conditions are met for 1 second.

#### P0134

• | DTCs P0068, P0101, P0102, P0103, P0106, P0107, P0108, P0112, P0113, P0116, P0117, P0118, P0120, P0121, P0122, P0123, P0128, P0201, P0202, P0203, P0204, P0205, P0206, P0207, P0208, P0220, P0222, P0223, P0442, P0443, P0446, P0449, P0455, P0496, P1516, P2101, P2119, P2135, P2176 are not set.

• | The Ignition 1 Signal parameter is between 10-18 volts.

• | The engine run time is more than 300 seconds.

• | DTC P0134 runs continuously when the above conditions are met.

#### P0140

• | DTCs P0068, P0101, P0102, P0103, P0106, P0107, P0108, P0112, P0113, P0116, P0117, P0118, P0120, P0121, P0122, P0123, P0128, P0201, P0202, P0203, P0204, P0205, P0206, P0207, P0208, P0220, P0222, P0223, P0442, P0443, P0446, P0449, P0455, P0496, P1516, P2101, P2119, P2135, P2176 are not set.

• | The Ignition 1 Signal parameter is between 10-18 volts.

• | The Engine Run Time parameter is more than 300 seconds.

• | The Loop Status parameter is closed.

• | DTC P0140 runs once per drive cycle when the above conditions are met.

#### P1133

• | DTCs P0068, P0101, P0102, P0103, P0106, P0107, P0108, P0112, P0113, P0116, P0117, P0118, P0120, P0121, P0122, P0123, P0128, P0201, P0202, P0203, P0204, P0205, P0206, P0207, P0208, P0220, P0222, P0223, P0442, P0443, P0446, P0449, P0455, P0496, P1516, P2101, P2119, P2135, P2176 are not set.

• | The ECT Sensor parameter is more than 60°C (140°F).

• | The Engine Speed parameter is between 1,200-3,000 RPM.

• | The Ignition 1 Signal parameter is between 10-18 volts.

• | The Engine Run Time parameter is more than 160 seconds.

• | The Loop Status parameter is Closed.

• | The TP Indicated Angle parameter is more than 5 percent.

• | The Fuel Level Sensor parameter is more than 10 percent.

• | The BARO Pressure parameter is more than 70 kPa.

• | The MAF Sensor parameter is between 20-55 g/s.

• | DTC P1133 runs once per drive cycle when the above conditions are met for 1 second.

#### P2270

• | DTCs P0036, P0037, P0038, P0137, P0138, P0140, P0141, P0443, P0458, P0459, P2232 are not set.

• | The Ignition 1 Signal parameter is between 10-18 volts.

• | The Engine Speed parameter is between 500-5,000 RPM.

• | The MAF Sensor parameter is between 3-50 g/s.

• | The Vehicle Speed parameter is between 24-132 km/h (15-82 mph).

• | The Fuel Level Sensor parameter is more than 10 percent.

• | The Loop Status parameter is closed.

• | DTC P2270 runs once per drive cycle when the above conditions are met.

#### P2271

• | DTCs P0036, P0037, P0038, P0137, P0138, P0140, P0141, P0443, P0458, P0459, P2232 are not set.

• | The Ignition 1 Signal parameter is between 10-18 volts.

• | The Engine Speed parameter is between 500-5,000 RPM.

• | The MAF Sensor parameter is between 3-50 g/s.

• | The Vehicle Speed parameter is between 24-132 km/h (15-82 mph).

• | The Fuel Level Sensor parameter is more than 10 percent.

• | The Loop Status parameter is closed.

• | DTC P2271 runs once per drive cycle when the above conditions are met for 1 second.

### Conditions for Setting the DTC

#### P0133

• | The ECM detects that the HO2S 1 rich-to-lean or lean-to-rich average response time is more than a calibrated value.

• | DTC P0133 sets within 100 seconds when the above condition is met.

#### P0134

• | The ECM detects that the HO2S 1 parameter is between 350-550 mV for 100 seconds.

• | The Throttle Position (TP) Indicated Angle parameter changes more than 5 percent, 1 time.

• | DTC P0134 sets within 100 seconds when the above conditions are met.

#### P0140

• | The ECM detects that the HO2S 1 parameter is between 410-490 mV.

• | The TP Indicated Angle parameter changes more than 5 percent 6 times.

• | DTC P0140 sets within 100 seconds when the above conditions are met.

#### P1133

• | The ECM detects that the HO2S 1 rich-to-lean counts, or the lean-to-rich counts are less than a calibrated value.

• | DTC P1133 sets within 100 seconds when the above condition is met.

#### P2270

• | The ECM detects that the HO2S 2 voltage oscillations are slower than a calibrated value.

• | DTC P2270 sets within 4 seconds when the above condition is met continuously, or within 50 seconds when the above condition is met cumulatively.

#### P2271

• | The ECM detects that the HO2S 2 voltage oscillations are faster than a calibrated value.

• | DTC P2271 sets within 4 seconds when the above condition is met continuously, or within 50 seconds when the above condition is met cumulatively.

### Action Taken When the DTC Sets

DTCs P0133, P0134, P0140, P1133, P2270, and P2271 are Type B DTCs.

### Conditions for Clearing the DTC

DTCs P0133, P0134, P0140, P1133, P2270, and P2271 are Type B DTCs.

### Reference Information

#### Schematic Reference

Engine Controls Schematics

#### Connector End View Reference

Component Connector End Views

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Heated Oxygen Sensor Wiring Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### DTC Type Reference

Powertrain Diagnostic Trouble Code (DTC) Type Definitions

#### Scan Tool Reference

Control Module References for scan tool information

### Circuit/System Verification

1. If any HO2S heater DTCs are set, perform those diagnostics first.
2. Allow the engine to reach operating temperature.
3. Engine running, observe the affected HO2S parameter with a scan tool.

• | The pre-catalyst oxygen sensors value should vary from below 200 mV to above 800 mV and respond to fueling changes.

• | The post-catalyst oxygen sensors value should change more than 200 mV when the throttle is quickly cycled 3 times from closed to wide open and back to closed after running the engine at 1,500 RPM for 30 seconds.

4. The affected HO2S may be damaged due to contamination. Prior to replacing the affected HO2S, inspect for the following sources of contamination:

Notice: Refer to Silicon Contamination of Heated Oxygen Sensors Notice in the Preface section.

• | A silicon contaminated HO2S

• | Fuel contamination--Refer to Alcohol/Contaminants-in-Fuel Diagnosis.

• | Engine oil consumption--Refer to Oil Consumption Diagnosis.

• | Engine coolant consumption--Refer to Loss of Coolant.

5. Operate the vehicle within the Conditions for Running the DTC to verify the DTC does not reset. You may also operate the vehicle within the conditions that you observed from the Freeze Frame/Failure Records data.

### Circuit/System Testing

Important: All modules must be powered down or misdiagnosis may result.

1. Ignition OFF, disconnect the scan tool and wait 60 seconds to ensure all modules are powered down.
2. Ignition OFF, disconnect the harness connector at the appropriate HO2S.
3. Ignition OFF, measure for less than 5 ohms between the appropriate HO2S low signal circuit terminal A and ground.

⇒ | If more than the specified range, test the appropriate HO2S low signal circuit for an open/high resistance. If the circuit tests normal, replace the ECM.

4. Ignition ON, verify the appropriate scan tool HO2S parameter is approximately 450 mV.

⇒ | If more than the specified value, test the appropriate HO2S high signal circuit for a short to voltage. If the circuit tests normal, replace the ECM.

⇒ | If less than the specified value, test the appropriate HO2S high signal circuit for a short to ground. If the circuit tests normal, replace the ECM.

5. Ignition ON, install a 3A fused jumper wire at the HO2S high signal circuit terminal B. Toggle the jumper wire between the HO2S low signal circuit terminal A and battery voltage. Verify the appropriate scan tool HO2S parameter toggles between 0 mV and approximately 1,000 mV.

⇒ | If the appropriate scan tool HO2S parameter does not toggle correctly, test the HO2S high signal circuit for an open/high resistance. If the circuits test normal, replace the ECM.

6. If all circuits test normal, replace the appropriate HO2S.

### Repair Instructions

Notice: Refer to Heated Oxygen and Oxygen Sensor Notice in the Preface section.

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

• | Heated Oxygen Sensor Replacement - Bank 1 Sensor 1

• | Heated Oxygen Sensor Replacement - Bank 1 Sensor 2

• | Control Module References for ECM replacement, setup, and programming