For 1990-2009 cars

### Removal Procedure

1. Remove the front seat head restraint. Refer to Front Seat Head Restraint Replacement .
2. Disengage the front head restraint cover J-strip by pulling the flap (1) back and out of flap (2) in the direction shown.
3. Pull out staples attaching cover side tabs.
4. Remove the front head restraint cover.

### Installation Procedure

1. Install the head restraint cover.
2. Use staples to secure cover side tabs.
3. Engage the front head restraint cover J-strip by inter locking the flap (1) with flap (2) in the direction shown.
4. Install the front seat head restraint. Refer to Front Seat Head Restraint Replacement .