For 1990-2009 cars

### Removal Procedure

Notice: Handle the electronic throttle control components carefully. Use cleanliness in order to prevent damage. Do not drop the electronic throttle control components. Do not roughly handle the electronic throttle control components. Do not immerse the electronic throttle control components in cleaning solvents of any type.

1. Remove the left instrument panel (I/P) on the lower closeout insulator panel. Refer to Knee Bolster Replacement.
2. Disconnect the electrical connector (1) to the accelerator pedal sensor module.
3. Remove the accelerator pedal to steering column support bracket retaining bolts (2).
4. Remove the accelerator pedal.

### Installation Procedure

1. Install the accelerator pedal to the steering column support bracket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the accelerator pedal to steering column support bracket retaining bolts (2).

Tighten
Tighten the accelerator pedal mounting bolts to 20 N·m (15 lb ft).

3. Connect the accelerator pedal sensor module electrical connector (1).
4. Inspect for correct carpet fit under the accelerator pedal.
5. If re-programming is required. Refer to Control Module References.
6. Install the left I/P on the lower closeout insulator panel. Refer to Knee Bolster Replacement.