For 1990-2009 cars

## Engine Ground Strap Replacement 3.6L Engine

### Removal Procedure

1. Ignition OFF.

Caution: Refer to Battery Disconnect Caution in the Preface section.

2. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
3. Remove the engine ground strap to the right side engine cylinder head retaining nut (1).
4. Remove the engine ground strap to ABS module mounting bracket retaining bolt (2).
5. Remove the engine ground strap from the vehicle.

### Installation Procedure

1. Position the engine ground strap to the correct position.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the engine ground strap to ABS module mounting bracket retaining bolt (2).

Tighten
Tighten the bolt to 15 N·m(11 lb ft).

3. Install the engine ground strap to the right side engine cylinder head retaining nut (1).

Tighten
Tighten the nut to 25 N·m(18 lb ft).

Caution: Refer to Battery Disconnect Caution in the Preface section.

4. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.

## Engine Ground Strap Replacement 6.0L Engine

### Removal Procedure

1. Ignition OFF.

Caution: Refer to Battery Disconnect Caution in the Preface section.

2. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
3. Remove the engine ground strap to the right side engine cylinder head retaining nut (1).
4. Remove the engine ground strap to ABS module mounting bracket retaining bolt (2).
5. Remove the engine ground strap from the vehicle.

### Installation Procedure

1. Position the engine ground strap to the correct position.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the engine ground strap to ABS module mounting bracket retaining bolt (2).

Tighten
Tighten the bolt to 15 N·m(11 lb ft).

3. Install the engine ground strap to the right side engine cylinder head retaining nut (1).

Tighten
Tighten the nut to 25 N·m(18 lb ft).

Caution: Refer to Battery Disconnect Caution in the Preface section.

4. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.