For 1990-2009 cars

### Removal Procedure

1. Disengage the I/P extension panel (1) to I/P carrier retaining clips (2).
2. Remove the I/P extension panel (1) from the centre console side trim panel (3).

### Installation Procedure

1. Align the I/P extension panel (1) with the I/P carrier.
2. Engage the I/P extension panel (1) to I/P carrier retaining clips (2).
3. Install the centre console side trim panel (3) to the I/Pextension panel (1).