For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

Important: Nuts with micro-encapsulated thread sealant must be discarded after removal.

2. Remove the stabiliser bar link to stabiliser bar retaining nut (1).

Discard the nut.

3. Disconnect the stabiliser bar link (3) from the stabiliser bar (2).
4. Remove and the stabiliser bar link to lower control arm retaining nut (5).

Discard the nut.

5. Remove the stabiliser bar link (3) from the lower control arm (4).
6. Remove the stabiliser bar link (3).
7. Inspect all parts for wear and damage.

### Installation Procedure

1. Connect the stabiliser bar link (3) to the stabiliser bar (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the stabiliser bar link to stabiliser bar NEW retaining nut (1).

Tighten
Tighten the nut to 50 N·m (37 lb ft).

3. Install the stabiliser bar link (3) to the lower control arm (4).
4. Install the stabiliser bar link to lower control arm retaining NEW nut (5).

Tighten
Tighten the nut to 50 N·m (37 lb ft).

5. Remove the safety stands.
6. Lower the vehicle to the ground.