For 1990-2009 cars

1. Remove the lifter guide (1) to cylinder block retaining bolts (2).
2. Remove the valve lifter guides (1) with valve lifters.

Important: Note the installed position of the guides. The notched area of the guide is to align with the locating tab on the block.

3. Remove the valve lifters (1) from the valve lifter guide (2).

Important: When using the valve train components again, always install the components to the original location and position. Refer to Separating Parts.