For 1990-2009 cars

#### Tools Required

• | DT-47721 Shift Shaft Seal Installer

• | DT-47722 Shift Rail Bushing Remover and Installer

• | DT-47723 Output Shaft Bearing Installer

• | DT-47724 Output Shaft Bearing Cup Installer

• | DT-47725 Extension Housing Bearing Cup Installer

• | DT-47726 Countershaft Rear Bearing Installer

### Rear Case Assemble

1. Apply gear oil to bearing. Use DT-47726 (1) to install bearing (2).
2. Install the bearing retainer (2) and bolt (1).

Tighten
Tighten the bolt to 11 N·m (96 lb in).

3. Install the gasket (3) to the rear case.
4. Install the oil trough (1) to the rear case.
5. Using DT-47722 (1), install the bearing (2) in the rear case.
6. Using DT-47724 , install the tapered bearing race (1) into the rear case.

### Middle Case Assemble

Using DT-47722 (1), install the bearing (2) in the intermediate case.