For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the left instrument panel lower trim plate (1) by pulling the panel down and disengaging the retaining clips.
3. Disconnect the electrical connectors (1) from the instrument panel compartment lamp switch.
4. Open the instrument panel compartment.

Important: Remove the instrument panel compartment lamp switch (1), by pushing it through the instrument panel compartment.

5. Remove the instrument panel compartment lamp switch (1).

### Installation Procedure

1. Install the instrument panel compartment lamp switch (1), listen for an audible click to confirm fitting.
2. Close the instrument panel compartment.
3. Connect the electrical connectors (1) to the instrument panel compartment lamp switch.
4. Install the left instrument panel lower trim plate (1) by engaging the instrument panel lower trim plate retaining clips.
5. Connect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection .
6. Test the operation of the instrument panel compartment lamp switch.