For 1990-2009 cars

### Removal Procedure

1. Remove the tonneau cover. Refer to Pickup Box Cover Replacement .
2. Remove the cargo liner to tie down bracket retaining bolts (2).
3. Remove the tie down brackets (1) from the cargo liner.
4. Remove the cargo liner to tail lamp filler panel retaining scrivets (1). Repeat for opposite side.
5. Remove the cargo liner to rear end panel retaining screws (1).

Important: Remove the cargo liner (1) by lifting the rear end of the cargo liner and sliding rearwards from the vehicle (2).

6. Remove the cargo liner (1) from the vehicle (2).

### Installation Procedure

Important: Install the cargo liner (1) by sliding the cargo liner forward and lowering the cargo liner to the rear of the vehicle (2).

1. Install the cargo liner (1) to the vehicle (2).
2. Align the cargo liner (1) to the rear most position of the vehicle body (2).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the cargo liner to rear end panel retaining screws (1).

Tighten
Tighten the screws to 1.5 N·m (13 lb in).

4. Install the cargo liner to tail lamp filler panel retaining scrivets (1). Repeat for opposite side.
5. Install the tie down brackets (1) to the cargo liner.
6. Install the cargo area to tie down bracket retaining bolts (2). Repeat for opposite side.

Tighten
Tighten the bolts to 22 N·m (16 lb ft).

7. Install the tonneau cover. Refer to Pickup Box Cover Replacement .