For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Caliper Anchor Plate Retaining Bolts

- First Pass

80 N·m

63 lb ft

- Final Pass

45 Degrees

Caster Arm to Steering Knuckle Retaining Nut

- First Pass

40 N·m

30 lb ft

- Final Pass

60 Degrees

Caster Arm to Sub Frame Retaining Bolt

- First Pass

50 N·m

37 lb ft

- Final Pass

120 Degrees

Front Brake Disc Splash Shield to Steering Knuckle Retaining Bolts | 9 N·m | 80 lb in
Front Caster Arm Ball Joint Retaining Nut

- First Pass

40 N·m

30 lb ft

- Final Pass

60 Degrees

Front Caster Arm Inner Pivot Retaining Bolt and Nut

- First Pass

50 N·m

37 lb ft

- Final Pass

120 Degrees

Front Subframe to Body Centre Retaining Bolts | 160 N·m | 118 lb ft
Front Subframe to Body Front Retaining Bolts | 160 N·m | 118 lb ft
Front Subframe to Body Rear Retaining Bolts | 240 N·m | 178 lb ft
Front Wheel Hub Assembly to Steering Knuckle Retaining Bolts | 108 N·m | 80 lb ft
Lower Control Arm Ball Joint Retaining Nut

- First Pass

40 N·m

30 lb ft

- Final Pass

60 Degrees

Lower Control Arm Inner Retaining Bolt

- First Pass

50 N·m

37 lb ft

- Final Pass

120 Degrees

Power Steering Gear Inlet Pipe/Hose Bracket to Sub Frame Retaining Bolt | 9 N·m | 80 lb in
Power Steering Gear Outlet Pipe/Hose Bracket to Sub Frame Retaining Bolt | 9 N·m | 80 lb in
Stabiliser Bar Link Ball Joint Stud Retaining Nuts | 50 N·m | 37 lb ft
Stabiliser Bar Support Bracket Retaining Nuts | 22 N·m | 16 lb ft
Steering Knuckle to Strut Assembly Retaining Bolts

- First Pass

85 N·m

63 lb ft

- Second Pass

100 N·m

74 lb ft

- Final Pass

90 Degrees

Strut Assembly Retaining Nut | 75 N·m | 55 lb ft
Strut Assembly to Body Retaining Nut | 55 N·m | 41 lb ft
Tie Rod to Steering Knuckle Retaining Nut | 70 N·m | 52 lb ft

### Front Spring Specifications

Suspension Configuration | Number of Coils | Free Length | Main Body Inside Diameter | Spring Rate | Production I.D Code
--- | --- | --- | --- | --- | ---
FE1 | 5.5 | 391 mm | 15.39 in | 146 mm | 5.75 in | 21 - 23 N/mm | 117 - 129 lb/in | AVA
FE2 | 5.1 | 358 mm | 14.09 in | 146 mm | 5.75 in | 23 - 26 N/mm | 129 - 145 lb/in | AVB
FR1 | 5.1 | 348 mm | 13.70 in | 146 mm | 5.75 in | 31 - 33 N/mm | 173 - 185 lb/in | AVC
HSV Maloo | 5.3 | 308 mm | 12.10 in | 146 mm | 5.74 in | 28 - 34 N/mm | - lb/in | N/A

### Front Stabiliser Bar Specifications

Suspension Configuration | Diameter mm (in) | Production I.D Code
--- | --- | ---
All | 23 mm (9.05 in) | XJ

### Front Strut Unit Specifications

Suspension Configuration | Left Side I.D Code | Right Side I.D Code
--- | --- | ---
FE1 | AM | AL
FE2 | AB | AA
FR1 | BSY | BSZ
HSV Maloo | ME | ME