For 1990-2009 cars

### Removal Procedure

Important: Take care not to damage the paint work when prying the endgate emblem (2) from the endgate (1).

1. Apply heat to the endgate emblem (2) with a heat gun to reduce the adhesion of the endgate emblem (2) to the endgate (1).

Important: Take care not to damage the paint work when prying the endgate emblem (2) from the endgate (1).

2. Use a suitable tool to carefully prise the endgate emblem (2) from the endgate (1)
3. Remove the endgate emblem (2) from the endgate (1).
4. Remove any remaining adhesive from the endgate and clean the surface with a suitable cleaning solution using a lint free cloth.

### Installation Procedure

Important: Use spec HN2021 or equivalent pressure sensitive double sided tape.

1. If reusing the endgate emblem, clean the endgate emblem with a suitable cleaning solution, using a lint free cloth.

Important: Do not allow the pressure sensitive double side tape to come in contact with any dirt or foreign material.

2. Apply new pressure sensitive double sided tape to the back of the endgate emblem (2).
3. Trim back the pressure sensitive double sided tape to the inner edge (1) of the endgate emblem (2).
4. Install the endgate emblem (2) to the endgate (3) into the correct position. Refer to Graphics/Decals/Emblems.
5. Firmly press the endgate emblem (2) to the endgate (1). Hold in position for 30 seconds.