For 1990-2009 cars

The Transmission Scan Tool Data List contains manual transmission related parameters that are available on the scan tool. The list is arranged in alphabetical order. A given parameter may appear in any one of the data lists, and in some cases may appear more than once, or in more than one data list in order to group certain related parameters together.

Use the Transmission Scan Tool Data List only after the following is determined:

• | The Diagnostic System Check - Vehicle in Vehicle DTC Information, is completed.

• | There are no diagnostic trouble codes (DTCs) shown.

• | The on-board diagnostics are functioning properly.

Scan tool values from a properly functioning vehicle may be used for comparison with the vehicle you are diagnosing.

Important: A scan tool that displays faulty data should not be used. The scan tool concern should be reported to the manufacturer. Use of a faulty scan tool can result in misdiagnosis and unnecessary parts replacement.

Only the parameters listed below are referenced in this service manual for use in diagnosis. If all values are within the typical range described below, refer to Symptoms - Manual Transmission in Manual Transmission - Aisin AY6.

The column labelled Data List indicates where a parameter can be located on the scan tool. Refer to the scan tool operating manual for the exact locations of the data lists. The following is a description of each term listed:

Engine Data 1: (1)
Engine Data 2: (2)
EVAP Data: (3)
Fuel Trim Data: (4)
HO2S Data: (5)
Misfire Data: (6)
TAC Data: (7)
CMP Actuator Data: (8)
Cooling/HVAC Data: (9)
Cruise/Traction Data: (10)
Electrical/Theft Data: (11)
IPC Data: (12)
ODM Data: (13)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Engine Idling/Radiator Hose Hot/Closed Throttle/Park or Neutral/Closed Loop/Accessories Off/Brake Pedal Released
CPP Switch (If Equipped) | 1 | APPLIED/RELEASED | RELEASED
Wheel Speed Sensor | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 12 | km/h (mph) | 0