For 1990-2009 cars

Cause | Correction
--- | ---
Incorrect oil filter without anti-drainback feature. | Install the correct oil filter. Refer to Engine Oil and Oil Filter Replacement .
Incorrect oil viscosity. | Install the correct viscosity oil. Refer to Engine Oil and Oil Filter Replacement .
High valve lifter leak down rate. | Replace the lifters, as required. Refer to Cylinder Head Replacement - Right Side .
Worn crankshaft thrust bearing. |

1. Check the crankshaft end play. Refer to Engine Mechanical Specifications .
2. Inspect the thrust bearing and crankshaft. Refer to Crankshaft and Bearing Cleaning and Inspection .
3. Repair or replace, as required. Refer to Crankshaft and Bearing Removal .

or

Refer to Crankshaft and Bearing Installation .