For 1990-2009 cars

## Floor Rear Air Outlet Duct Replacement - Right Side RHD

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Remove the front carpet. Refer to Front Floor Panel Carpet Replacement.
2. Remove the centre console. Refer to Front Floor Console Replacement.
3. Remove the push pins (2) from the rear floor air outlet duct (1).
4. Remove the rear floor air outlet duct (1) from the floor (2).
5. Disconnect the rear floor air outlet duct (1) from the HVAC module assembly (2).

### Installation Procedure

1. Install the rear floor air outlet duct (1) to the HVAC module assembly (2).
2. Install the rear floor air outlet duct (1) to the floor (2).
3. Install the push pins (2) to the rear floor air outlet duct (1).
4. Install the centre console. Refer to Front Floor Console Replacement.
5. Install the front carpet. Refer to Front Floor Panel Carpet Replacement.