For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear wheels. Refer to Tire and Wheel Removal and Installation .
3. Remove the rear strut assembly. Refer to Strut Assembly Replacement .
4. Remove the rear strut assembly support mount. Refer to Rear Suspension Strut Mount Replacement .
5. Remove the rear coil spring. Refer to Coil Spring Replacement .
6. Remove the shock absorber (1) from the mounting trestle, or vice.
7. Inspect all parts for wear and damage.

### Installation Procedure

Notice: Refer to General Repair Instructions in the Preface section.

1. Mount the shock absorber (1) on a mounting trestle, or a vice.
2. Install the rear coil spring. Refer to Coil Spring Replacement .
3. Install the rear strut assembly support mount. Refer to Rear Suspension Strut Mount Replacement .
4. Install the rear strut assembly. Refer to Strut Assembly Replacement .
5. Install the rear wheel. Refer to Tire and Wheel Removal and Installation .
6. Remove the safety stands.
7. Lower the vehicle to the ground.