For 1990-2009 cars

Callout | Component Name
--- | ---
1 | 4-5-6 Clutch Dampener Retaining Ring Notice: Refer to General Repair Instructions in the Preface section.
2 | 4-5-6 Clutch Dampener Apply Plate
3 | 4-5-6 Clutch Dampener Tip Dry and inspect the clutch dampener for the following conditions:

• | Pitting

• | Flaking

• | Delamination

• | Wear

• | Glazing

• | Cracking

If any of these conditions are found, replace the dampener.