For 1990-2009 cars

## Secondary Driver Information DisplayDescription and Operation HSV Maloo

### Engine Oil Temperature Gauge

The SIC gauges display the engine oil temperature as determined by the SIC module. The oil temperature gauge will default to 0 if:

• | The SIC module detects loss of oil temperature signal.

• | The SIC module detects a malfunction in the engine oil temperature sensor circuit.

### Engine Oil Pressure Gauge

The SIC gauges display the engine oil pressure as determined by the SIC module. The oil pressure gauge will default to 0 if:

• | The SIC module detects a malfunction in the engine oil pressure sensor circuit.

• | The SIC module detects a loss of pressure in the engine oil circuit.

• | The SIC module detects loss of oil pressure signal.

### Voltage Gauge

The SIC gauges display the vehicle voltage as determined by the SIC module. The voltage gauge will default to 0 if:

• | The SIC module detects a malfunction in the engine charging system.

• | The SIC module detects loss of voltage signal.