For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Important: The manual shaft must be removed to replace the manual shaft seal. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the transmission from the vehicle. Refer to Transmission Replacement .
3. Remove the transmission fluid pan. Refer to Automatic Transmission Fluid, Fluid Pan and/or Filter Replacement .
4. Remove the control valve body. Refer to Control Valve Lower Body and Upper Body Replacement

1 | Manual Shift Shaft Pin

#### Tip

• | Discard the pin. Replace with NEW pin.

• | "Walk" the pin out using side cutters.

2 | Manual Shaft Detent Lever Hub Pin

#### Tip

• | Discard the pin. Replace with NEW pin.

• | "Walk" the pin out using side cutters.

3 | Manual Shift Shaft
4 | Manual Shift Shaft Seal

#### Tip

• | Use the J 45201 to remove the seal from the transmission case.

• | Use the J 43909 to install the seal into the transmission case.