For 1990-2009 cars

## Instrument Panel Compartment Door Lock Cylinder Latch Retainer Replacement RHD

### Removal Procedure

1. Remove the close out panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.
2. Remove the instrument panel outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement.
3. Remove the instrument panel compartment. Refer to Instrument Panel Compartment Replacement.
4. Remove the instrument panel compartment door latch release handle. Refer to Instrument Panel Compartment Door Latch Release Handle Replacement.
5. Using a suitable tool, disengage the retention tabs (1) from the instrument panel compartment door latch release handle (2), expelling the instrument panel compartment door lock cylinder latch retainer (3).

### Installation Procedure

1. Install the instrument panel compartment door lock cylinder latch retainer (3) into the instrument panel compartment door latch release handle (2), engaging the retention tabs (1).
2. Install the instrument panel compartment door latch release handle. Refer to Instrument Panel Compartment Door Latch Release Handle Replacement.
3. Install the instrument panel compartment. Refer to Instrument Panel Compartment Replacement.
4. Install the instrument panel outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement.
5. Install the close out panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.

## Instrument Panel Compartment Door Lock Cylinder Latch Retainer Replacement LHD

### Removal Procedure

1. Remove the instrument panel insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.
2. Remove the instrument panel outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement.
3. Remove the instrument panel compartment. Refer to Instrument Panel Compartment Replacement.
4. Remove the instrument panel compartment door latch release handle. Refer to Instrument Panel Compartment Door Latch Release Handle Replacement.
5. Using a suitable tool, disengage the retention tabs (1) from the instrument panel compartment door latch release handle (2), expelling the instrument panel compartment door lock cylinder latch retainer (3).

### Installation Procedure

1. Install the instrument panel compartment door lock cylinder latch retainer (3) into the instrument panel compartment door latch release handle (2), engaging the retention tabs (1).
2. Install the instrument panel compartment door latch release handle. Refer to Instrument Panel Compartment Door Latch Release Handle Replacement.
3. Install the instrument panel compartment. Refer to Instrument Panel Compartment Replacement.
4. Install the instrument panel outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement.
5. Install the instrument panel insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.