For 1990-2009 cars

## Drive Belt Idler Pulley Installation With Air Condictioning

1. Install the dished washer (4) and drive belt idler pulley (3) to the accessory drive mounting bracket (2).
2. Hand tighten the drive belt idler pulley to accessory drive mounting bracket retaining bolt (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Tighten the drive belt idler pulley to accessory drive mounting bracket retaining bolt (1).

Tighten
Tighten the bolt to 22 N·m (16 lb ft).