For 1990-2009 cars

### Removal Procedure

1. Remove the air intake duct. Refer to Air Cleaner Assembly Replacement.
2. Remove the accessory drive belt. Refer to Drive Belt Replacement - Accessory.
3. Remove the drive belt idler pulley to alternator bracket retaining bolt (1).
4. Remove the drive belt idler pulley (2).

### Installation Procedure

1. Install the drive belt idler pulley (2).
2. Hand tighten the drive belt idler pulley to alternator bracket retaining bolt (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Tighten the drive belt idler pulley bolt.

Tighten
Tighten the bolt to 58 N·m (43 lb ft).

4. Install the accessory drive belt. Refer to Drive Belt Replacement - Accessory.
5. Install the air intake duct. Refer to Air Cleaner Assembly Replacement.