For 1990-2009 cars

### Removal Procedure - Right

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Brake Dust Caution in the Preface section.

1. Disconnect the wheel speed sensor jumper harness electrical connector (1).
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
3. Remove the right hand front wheel. Refer to Tire and Wheel Removal and Installation .
4. Disconnect the wheel speed sensor jumper harness electrical connector (4).
5. Detach the wheel speed sensor jumper harness (2) from the brake hose/wheel speed sensor jumper harness bracket (1).
6. Detach the wheel speed sensor jumper harness (2) from the front strut mounting bracket (3).

Important: Note the routing of the wheel speed sensor jumper harness (2).

7. Remove the wheel speed sensor jumper harness (2) from the vehicle.

### Installation Procedure - Right

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Brake Dust Caution in the Preface section.

Important: Make sure the routing of the wheel speed sensor jumper harness (2) is secured and routed in its original location.

1. Install the wheel speed sensor jumper harness (2) to the vehicle.
2. Attach the wheel speed sensor jumper harness (2) from the front strut mounting bracket (3).
3. Attach the wheel speed sensor jumper harness (2) to the brake hose/wheel speed sensor jumper harness bracket (1).
4. Connect the wheel speed sensor jumper harness electrical connector (4).
5. Install the right hand front wheel. Refer to Tire and Wheel Removal and Installation .
6. Lower the vehicle.
7. Connect the wheel speed sensor jumper harness electrical connector (1).
8. Use the scan tool in order to clear any DTCs.
9. Perform the System Check-Vehicle. Refer to Diagnostic System Check - Vehicle .

### Removal Procedure - Left

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Brake Dust Caution in the Preface section.

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement for 3.6L engine, or Air Cleaner Assembly Replacement for 6.0L engine.
2. Disconnect the wheel speed sensor jumper harness electrical connector (1).
3. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
4. Remove the left hand front wheel. Refer to Tire and Wheel Removal and Installation .
5. Disconnect the wheel speed sensor jumper harness electrical connector (1).
6. Detach the wheel speed sensor jumper harness (3) from the brake hose/wheel speed sensor jumper harness bracket (4).
7. Detach the wheel speed sensor jumper harness (3) from the front strut mounting bracket (2).

Important: Note the routing of the wheel speed sensor jumper harness (3).

8. Remove the wheel speed sensor jumper harness (3) from the vehicle.

### Installation Procedure - Left

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Brake Dust Caution in the Preface section.

Important: Make sure the routing of the wheel speed sensor jumper harness (3) is secured and routed in its original location.

1. Install the wheel speed sensor jumper harness (3) to the vehicle.
2. Attach the wheel speed sensor jumper harness (3) from the front strut mounting bracket (2).
3. Attach the wheel speed sensor jumper harness (3) to the brake hose/wheel speed sensor jumper harness bracket (4).
4. Connect the wheel speed sensor jumper harness electrical connector (1).
5. Install the left hand front wheel. Refer to Tire and Wheel Removal and Installation .
6. Lower the vehicle.
7. Connect the wheel speed sensor jumper harness electrical connector (1).
8. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement for 3.6L engine, or Air Cleaner Assembly Replacement for 6.0L engine.
9. Use the scan tool in order to clear any DTCs.
10. Perform the System Check-Vehicle. Refer to Diagnostic System Check - Vehicle .