For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Remove the rear frame. Refer to Rear Frame Replacement.
2. Disconnect the evaporative emission (EVAP) hoses (1&3) from the EVAP canister.
3. Remove the purge canister to chassis retaining bolts (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the purge canister to chassis retaining bolts (2).

Tighten
Tighten the EVAP canister retaining nuts to 6 N·m (53 lb in).

2. Connect the evaporative emission (EVAP) hoses (1&3) from the EVAP canister.
3. Install the rear frame. Refer to Rear Frame Replacement.