For 1990-2009 cars

1. Remove the spark plug leads (1).
2. Remove the ignition coil bracket retaining studs (2).
3. Remove the ignition coil and bracket assembly (1).
4. Remove the valve rocker arm cover retaining bolts (2) and valve rocker arm cover (1).

Important: The valve rocker arm cover gasket is a single use only component and must be replaced whenever the valve rocker arm cover is removed from the cylinder head.

5. Remove the valve rocker arm cover gasket (1).

Discard the valve rocker arm cover gasket (1).